#include "skeleton.dtsi"

/ {
	model = "Atmel SAMA5D2 family SoC";
	compatible = "atmel,sama5d2";

	aliases {
		spi0 = &spi0;
		spi1 = &qspi0;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
	};

	clocks {
		slow_xtal: slow_xtal {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};

		main_xtal: main_xtal {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};
	};

	ahb {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;

		usb1: ohci@00400000 {
			compatible = "atmel,at91rm9200-ohci", "usb-ohci";
			reg = <0x00400000 0x100000>;
			clocks = <&uhphs_clk>, <&uhphs_clk>, <&uhpck>;
			clock-names = "ohci_clk", "hclk", "uhpck";
			status = "disabled";
		};

		usb2: ehci@00500000 {
			compatible = "atmel,at91sam9g45-ehci", "usb-ehci";
			reg = <0x00500000 0x100000>;
			clocks = <&utmi>, <&uhphs_clk>;
			clock-names = "usb_clk", "ehci_clk";
			status = "disabled";
		};

		sdmmc0: sdio-host@a0000000 {
			compatible = "atmel,sama5d2-sdhci";
			reg = <0xa0000000 0x300>;
			clocks = <&sdmmc0_hclk>, <&sdmmc0_gclk>, <&main>;
			clock-names = "hclock", "multclk", "baseclk";
			status = "disabled";
		};

		sdmmc1: sdio-host@b0000000 {
			compatible = "atmel,sama5d2-sdhci";
			reg = <0xb0000000 0x300>;
			clocks = <&sdmmc1_hclk>, <&sdmmc1_gclk>, <&main>;
			clock-names = "hclock", "multclk", "baseclk";
			status = "disabled";
		};

		apb {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;

			pmc: pmc@f0014000 {
				compatible = "atmel,sama5d2-pmc", "syscon";
				reg = <0xf0014000 0x160>;
				#address-cells = <1>;
				#size-cells = <0>;
				#interrupt-cells = <1>;

				main: mainck {
					compatible = "atmel,at91sam9x5-clk-main";
					#clock-cells = <0>;
				};

				plla: pllack@0 {
					compatible = "atmel,sama5d3-clk-pll";
					#clock-cells = <0>;
					clocks = <&main>;
					reg = <0>;
					atmel,clk-input-range = <12000000 12000000>;
					#atmel,pll-clk-output-range-cells = <4>;
					atmel,pll-clk-output-ranges = <600000000 1200000000 0 0>;
				};

				plladiv: plladivck {
					compatible = "atmel,at91sam9x5-clk-plldiv";
					#clock-cells = <0>;
					clocks = <&plla>;
				};

				audio_pll_frac: audiopll_fracck {
					compatible = "atmel,sama5d2-clk-audio-pll-frac";
					#clock-cells = <0>;
					clocks = <&main>;
				};

				audio_pll_pad: audiopll_padck {
					compatible = "atmel,sama5d2-clk-audio-pll-pad";
					#clock-cells = <0>;
					clocks = <&audio_pll_frac>;
				};

				audio_pll_pmc: audiopll_pmcck {
					compatible = "atmel,sama5d2-clk-audio-pll-pmc";
					#clock-cells = <0>;
					clocks = <&audio_pll_frac>;
				};

				utmi: utmick {
					compatible = "atmel,at91sam9x5-clk-utmi";
					#clock-cells = <0>;
					clocks = <&main>;
				};

				mck: masterck {
					compatible = "atmel,at91sam9x5-clk-master";
					#clock-cells = <0>;
					clocks = <&main>, <&plladiv>, <&utmi>;
					atmel,clk-output-range = <124000000 166000000>;
					atmel,clk-divisors = <1 2 4 3>;
				};

				h32ck: h32mxck {
					#clock-cells = <0>;
					compatible = "atmel,sama5d4-clk-h32mx";
					clocks = <&mck>;
				};

				usb: usbck {
					compatible = "atmel,at91sam9x5-clk-usb";
					#clock-cells = <0>;
					clocks = <&plladiv>, <&utmi>;
				};

				prog: progck {
					compatible = "atmel,at91sam9x5-clk-programmable";
					#address-cells = <1>;
					#size-cells = <0>;
					interrupt-parent = <&pmc>;
					clocks = <&main>, <&plladiv>, <&utmi>, <&mck>;

					prog0: prog@0 {
						#clock-cells = <0>;
						reg = <0>;
					};

					prog1: prog@1 {
						#clock-cells = <0>;
						reg = <1>;
					};

					prog2: prog@2 {
						#clock-cells = <0>;
						reg = <2>;
					};
				};

				systemck {
					compatible = "atmel,at91rm9200-clk-system";
					#address-cells = <1>;
					#size-cells = <0>;

					ddrck: ddrck@2 {
						#clock-cells = <0>;
						reg = <2>;
						clocks = <&mck>;
					};

					lcdck: lcdck@3 {
						#clock-cells = <0>;
						reg = <3>;
						clocks = <&mck>;
					};

					uhpck: uhpck@6 {
						#clock-cells = <0>;
						reg = <6>;
						clocks = <&usb>;
					};

					udpck: udpck@7 {
						#clock-cells = <0>;
						reg = <7>;
						clocks = <&usb>;
					};

					pck0: pck0@8 {
						#clock-cells = <0>;
						reg = <8>;
						clocks = <&prog0>;
					};

					pck1: pck1@9 {
						#clock-cells = <0>;
						reg = <9>;
						clocks = <&prog1>;
					};

					pck2: pck2@10 {
						#clock-cells = <0>;
						reg = <10>;
						clocks = <&prog2>;
					};

					iscck: iscck@18 {
						#clock-cells = <0>;
						reg = <18>;
						clocks = <&mck>;
					};
				};

				periph32ck {
					compatible = "atmel,at91sam9x5-clk-peripheral";
					#address-cells = <1>;
					#size-cells = <0>;
					clocks = <&h32ck>;

					macb0_clk: macb0_clk@5 {
						#clock-cells = <0>;
						reg = <5>;
						atmel,clk-output-range = <0 83000000>;
					};

					tdes_clk: tdes_clk@11 {
						#clock-cells = <0>;
						reg = <11>;
						atmel,clk-output-range = <0 83000000>;
					};

					matrix1_clk: matrix1_clk@14 {
						#clock-cells = <0>;
						reg = <14>;
					};

					hsmc_clk: hsmc_clk@17 {
						#clock-cells = <0>;
						reg = <17>;
					};

					pioA_clk: pioA_clk@18 {
						#clock-cells = <0>;
						reg = <18>;
						atmel,clk-output-range = <0 83000000>;
					};

					flx0_clk: flx0_clk@19 {
						#clock-cells = <0>;
						reg = <19>;
						atmel,clk-output-range = <0 83000000>;
					};

					flx1_clk: flx1_clk@20 {
						#clock-cells = <0>;
						reg = <20>;
						atmel,clk-output-range = <0 83000000>;
					};

					flx2_clk: flx2_clk@21 {
						#clock-cells = <0>;
						reg = <21>;
						atmel,clk-output-range = <0 83000000>;
					};

					flx3_clk: flx3_clk@22 {
						#clock-cells = <0>;
						reg = <22>;
						atmel,clk-output-range = <0 83000000>;
					};

					flx4_clk: flx4_clk@23 {
						#clock-cells = <0>;
						reg = <23>;
						atmel,clk-output-range = <0 83000000>;
					};

					uart0_clk: uart0_clk@24 {
						#clock-cells = <0>;
						reg = <24>;
						atmel,clk-output-range = <0 83000000>;
					};

					uart1_clk: uart1_clk@25 {
						#clock-cells = <0>;
						reg = <25>;
						atmel,clk-output-range = <0 83000000>;
					};

					uart2_clk: uart2_clk@26 {
						#clock-cells = <0>;
						reg = <26>;
						atmel,clk-output-range = <0 83000000>;
					};

					uart3_clk: uart3_clk@27 {
						#clock-cells = <0>;
						reg = <27>;
						atmel,clk-output-range = <0 83000000>;
					};

					uart4_clk: uart4_clk@28 {
						#clock-cells = <0>;
						reg = <28>;
						atmel,clk-output-range = <0 83000000>;
					};

					twi0_clk: twi0_clk@29 {
						reg = <29>;
						#clock-cells = <0>;
						atmel,clk-output-range = <0 83000000>;
					};

					twi1_clk: twi1_clk@30 {
						#clock-cells = <0>;
						reg = <30>;
						atmel,clk-output-range = <0 83000000>;
					};

					spi0_clk: spi0_clk@33 {
						#clock-cells = <0>;
						reg = <33>;
						atmel,clk-output-range = <0 83000000>;
					};

					spi1_clk: spi1_clk@34 {
						#clock-cells = <0>;
						reg = <34>;
						atmel,clk-output-range = <0 83000000>;
					};

					tcb0_clk: tcb0_clk@35 {
						#clock-cells = <0>;
						reg = <35>;
						atmel,clk-output-range = <0 83000000>;
					};

					tcb1_clk: tcb1_clk@36 {
						#clock-cells = <0>;
						reg = <36>;
						atmel,clk-output-range = <0 83000000>;
					};

					pwm_clk: pwm_clk@38 {
						#clock-cells = <0>;
						reg = <38>;
						atmel,clk-output-range = <0 83000000>;
					};

					adc_clk: adc_clk@40 {
						#clock-cells = <0>;
						reg = <40>;
						atmel,clk-output-range = <0 83000000>;
					};

					uhphs_clk: uhphs_clk@41 {
						#clock-cells = <0>;
						reg = <41>;
						atmel,clk-output-range = <0 83000000>;
					};

					udphs_clk: udphs_clk@42 {
						#clock-cells = <0>;
						reg = <42>;
						atmel,clk-output-range = <0 83000000>;
					};

					ssc0_clk: ssc0_clk@43 {
						#clock-cells = <0>;
						reg = <43>;
						atmel,clk-output-range = <0 83000000>;
					};

					ssc1_clk: ssc1_clk@44 {
						#clock-cells = <0>;
						reg = <44>;
						atmel,clk-output-range = <0 83000000>;
					};

					trng_clk: trng_clk@47 {
						#clock-cells = <0>;
						reg = <47>;
						atmel,clk-output-range = <0 83000000>;
					};

					pdmic_clk: pdmic_clk@48 {
						#clock-cells = <0>;
						reg = <48>;
						atmel,clk-output-range = <0 83000000>;
					};

					i2s0_clk: i2s0_clk@54 {
						#clock-cells = <0>;
						reg = <54>;
						atmel,clk-output-range = <0 83000000>;
					};

					i2s1_clk: i2s1_clk@55 {
						#clock-cells = <0>;
						reg = <55>;
						atmel,clk-output-range = <0 83000000>;
					};

					can0_clk: can0_clk@56 {
						#clock-cells = <0>;
						reg = <56>;
						atmel,clk-output-range = <0 83000000>;
					};

					can1_clk: can1_clk@57 {
						#clock-cells = <0>;
						reg = <57>;
						atmel,clk-output-range = <0 83000000>;
					};

					classd_clk: classd_clk@59 {
						#clock-cells = <0>;
						reg = <59>;
						atmel,clk-output-range = <0 83000000>;
					};
				};

				periph64ck {
					compatible = "atmel,at91sam9x5-clk-peripheral";
					#address-cells = <1>;
					#size-cells = <0>;
					clocks = <&mck>;

					dma0_clk: dma0_clk@6 {
						#clock-cells = <0>;
						reg = <6>;
					};

					dma1_clk: dma1_clk@7 {
						#clock-cells = <0>;
						reg = <7>;
					};

					aes_clk: aes_clk@9 {
						#clock-cells = <0>;
						reg = <9>;
					};

					aesb_clk: aesb_clk@10 {
						#clock-cells = <0>;
						reg = <10>;
					};

					sha_clk: sha_clk@12 {
						#clock-cells = <0>;
						reg = <12>;
					};

					mpddr_clk: mpddr_clk@13 {
						#clock-cells = <0>;
						reg = <13>;
					};

					matrix0_clk: matrix0_clk@15 {
						#clock-cells = <0>;
						reg = <15>;
					};

					sdmmc0_hclk: sdmmc0_hclk@31 {
						#clock-cells = <0>;
						reg = <31>;
					};

					sdmmc1_hclk: sdmmc1_hclk@32 {
						#clock-cells = <0>;
						reg = <32>;
					};

					lcdc_clk: lcdc_clk@45 {
						#clock-cells = <0>;
						reg = <45>;
					};

					isc_clk: isc_clk@46 {
						#clock-cells = <0>;
						reg = <46>;
					};

					qspi0_clk: qspi0_clk@52 {
						#clock-cells = <0>;
						reg = <52>;
					};

					qspi1_clk: qspi1_clk@53 {
						#clock-cells = <0>;
						reg = <53>;
					};
				};

				gck {
					compatible = "atmel,sama5d2-clk-generated";
					#address-cells = <1>;
					#size-cells = <0>;
					interrupt-parent = <&pmc>;
					clocks = <&main>, <&plla>, <&utmi>, <&mck>;

					sdmmc0_gclk: sdmmc0_gclk@31 {
						#clock-cells = <0>;
						reg = <31>;
					};

					sdmmc1_gclk: sdmmc1_gclk@32 {
						#clock-cells = <0>;
						reg = <32>;
					};

					tcb0_gclk: tcb0_gclk@35 {
						#clock-cells = <0>;
						reg = <35>;
						atmel,clk-output-range = <0 83000000>;
					};

					tcb1_gclk: tcb1_gclk@36 {
						#clock-cells = <0>;
						reg = <36>;
						atmel,clk-output-range = <0 83000000>;
					};

					pwm_gclk: pwm_gclk@38 {
						#clock-cells = <0>;
						reg = <38>;
						atmel,clk-output-range = <0 83000000>;
					};

					pdmic_gclk: pdmic_gclk@48 {
						#clock-cells = <0>;
						reg = <48>;
					};

					i2s0_gclk: i2s0_gclk@54 {
						#clock-cells = <0>;
						reg = <54>;
					};

					i2s1_gclk: i2s1_gclk@55 {
						#clock-cells = <0>;
						reg = <55>;
					};

					can0_gclk: can0_gclk@56 {
						#clock-cells = <0>;
						reg = <56>;
						atmel,clk-output-range = <0 80000000>;
					};

					can1_gclk: can1_gclk@57 {
						#clock-cells = <0>;
						reg = <57>;
						atmel,clk-output-range = <0 80000000>;
					};

					classd_gclk: classd_gclk@59 {
						#clock-cells = <0>;
						reg = <59>;
						atmel,clk-output-range = <0 100000000>;
					};
				};
			};

			qspi0: spi@f0020000 {
				compatible = "atmel,sama5d2-qspi";
				reg = <0xf0020000 0x100>, <0xd0000000 0x08000000>;
				reg-names = "qspi_base", "qspi_mmap";
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&qspi0_clk>;
				status = "disabled";
			};

			spi0: spi@f8000000 {
				compatible = "atmel,at91rm9200-spi";
				reg = <0xf8000000 0x100>;
				clocks = <&spi0_clk>;
				clock-names = "spi_clk";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};

			macb0: ethernet@f8008000 {
				compatible = "cdns,macb";
				reg = <0xf8008000 0x1000>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&macb0_clk>, <&macb0_clk>;
				clock-names = "hclk", "pclk";
				status = "disabled";
			};

			uart1: serial@f8020000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf8020000 0x100>;
				status = "disabled";
			};

			i2c0: i2c@f8028000 {
				compatible = "atmel,sama5d2-i2c";
				reg = <0xf8028000 0x100>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&twi0_clk>;
				status = "disabled";
			};

			sckc@f8048050 {
				compatible = "atmel,at91sam9x5-sckc";
				reg = <0xf8048050 0x4>;

				slow_rc_osc: slow_rc_osc {
					compatible = "atmel,at91sam9x5-clk-slow-rc-osc";
					#clock-cells = <0>;
					clock-frequency = <32768>;
					clock-accuracy = <250000000>;
					atmel,startup-time-usec = <75>;
				};

				slow_osc: slow_osc {
					compatible = "atmel,at91sam9x5-clk-slow-osc";
					#clock-cells = <0>;
					clocks = <&slow_xtal>;
					atmel,startup-time-usec = <1200000>;
				};

				clk32k: slowck {
					compatible = "atmel,at91sam9x5-clk-slow";
					#clock-cells = <0>;
					clocks = <&slow_rc_osc &slow_osc>;
				};
			};

			spi1: spi@fc000000 {
				compatible = "atmel,at91rm9200-spi";
				reg = <0xfc000000 0x100>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};

			i2c1: i2c@fc028000 {
				compatible = "atmel,sama5d2-i2c";
				reg = <0xfc028000 0x100>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&twi1_clk>;
				status = "disabled";
			};

			pioA: gpio@fc038000 {
				compatible = "atmel,sama5d2-gpio";
				reg = <0xfc038000 0x600>;
				clocks = <&pioA_clk>;
				gpio-controller;
				#gpio-cells = <2>;

				pinctrl {
					compatible = "atmel,sama5d2-pinctrl";
				};
			};
		};
	};
};
