/*
 * Device Tree Source for UniPhier sLD3 SoC
 *
 * Copyright (C) 2015-2016 Socionext Inc.
 *   Author: Masahiro Yamada <yamada.masahiro@socionext.com>
 *
 * SPDX-License-Identifier:	GPL-2.0+	X11
 */

/include/ "skeleton.dtsi"

/ {
	compatible = "socionext,uniphier-sld3";

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			reg = <0>;
			enable-method = "psci";
			next-level-cache = <&l2>;
		};

		cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			reg = <1>;
			enable-method = "psci";
			next-level-cache = <&l2>;
		};
	};

	psci {
		compatible = "arm,psci-0.2";
		method = "smc";
	};

	clocks {
		refclk: ref {
			#clock-cells = <0>;
			compatible = "fixed-clock";
			clock-frequency = <24576000>;
		};

		arm_timer_clk: arm_timer_clk {
			#clock-cells = <0>;
			compatible = "fixed-clock";
			clock-frequency = <50000000>;
		};
	};

	soc {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		interrupt-parent = <&intc>;
		u-boot,dm-pre-reloc;

		timer@20000200 {
			compatible = "arm,cortex-a9-global-timer";
			reg = <0x20000200 0x20>;
			interrupts = <1 11 0x304>;
			clocks = <&arm_timer_clk>;
		};

		timer@20000600 {
			compatible = "arm,cortex-a9-twd-timer";
			reg = <0x20000600 0x20>;
			interrupts = <1 13 0x304>;
			clocks = <&arm_timer_clk>;
		};

		intc: interrupt-controller@20001000 {
			compatible = "arm,cortex-a9-gic";
			#interrupt-cells = <3>;
			interrupt-controller;
			reg = <0x20001000 0x1000>,
			      <0x20000100 0x100>;
		};

		l2: l2-cache@500c0000 {
			compatible = "socionext,uniphier-system-cache";
			reg = <0x500c0000 0x2000>, <0x503c0100 0x4>,
			      <0x506c0000 0x400>;
			interrupts = <0 174 4>, <0 175 4>;
			cache-unified;
			cache-size = <(512 * 1024)>;
			cache-sets = <256>;
			cache-line-size = <128>;
			cache-level = <2>;
		};

		serial0: serial@54006800 {
			compatible = "socionext,uniphier-uart";
			status = "disabled";
			reg = <0x54006800 0x40>;
			interrupts = <0 33 4>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_uart0>;
			clock-frequency = <36864000>;
		};

		serial1: serial@54006900 {
			compatible = "socionext,uniphier-uart";
			status = "disabled";
			reg = <0x54006900 0x40>;
			interrupts = <0 35 4>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_uart1>;
			clock-frequency = <36864000>;
		};

		serial2: serial@54006a00 {
			compatible = "socionext,uniphier-uart";
			status = "disabled";
			reg = <0x54006a00 0x40>;
			interrupts = <0 37 4>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_uart2>;
			clock-frequency = <36864000>;
		};

		port0x: gpio@55000008 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000008 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port1x: gpio@55000010 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000010 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port2x: gpio@55000018 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000018 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port3x: gpio@55000020 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000020 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port4: gpio@55000028 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000028 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port5x: gpio@55000030 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000030 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port6x: gpio@55000038 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000038 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port7x: gpio@55000040 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000040 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port8x: gpio@55000048 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000048 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port9x: gpio@55000050 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000050 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port10x: gpio@55000058 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000058 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port11x: gpio@55000060 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000060 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port12x: gpio@55000068 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000068 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port13x: gpio@55000070 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000070 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port14x: gpio@55000078 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000078 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		port16x: gpio@55000088 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000088 0x8>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		i2c0: i2c@58400000 {
			compatible = "socionext,uniphier-i2c";
			status = "disabled";
			reg = <0x58400000 0x40>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <0 41 1>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_i2c0>;
			clocks = <&sys_clk 1>;
			clock-frequency = <100000>;
		};

		i2c1: i2c@58480000 {
			compatible = "socionext,uniphier-i2c";
			status = "disabled";
			reg = <0x58480000 0x40>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <0 42 1>;
			clocks = <&sys_clk 1>;
			clock-frequency = <100000>;
		};

		i2c2: i2c@58500000 {
			compatible = "socionext,uniphier-i2c";
			status = "disabled";
			reg = <0x58500000 0x40>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <0 43 1>;
			clocks = <&sys_clk 1>;
			clock-frequency = <100000>;
		};

		i2c3: i2c@58580000 {
			compatible = "socionext,uniphier-i2c";
			status = "disabled";
			reg = <0x58580000 0x40>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <0 44 1>;
			clocks = <&sys_clk 1>;
			clock-frequency = <100000>;
		};

		/* chip-internal connection for DMD */
		i2c4: i2c@58600000 {
			compatible = "socionext,uniphier-i2c";
			reg = <0x58600000 0x40>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <0 45 1>;
			clocks = <&sys_clk 1>;
			clock-frequency = <400000>;
		};

		system_bus: system-bus@58c00000 {
			compatible = "socionext,uniphier-system-bus";
			status = "disabled";
			reg = <0x58c00000 0x400>;
			#address-cells = <2>;
			#size-cells = <1>;
		};

		smpctrl@59800000 {
			compatible = "socionext,uniphier-smpctrl";
			reg = <0x59801000 0x400>;
		};

		mioctrl@59810000 {
			compatible = "socionext,uniphier-mioctrl",
				     "simple-mfd", "syscon";
			reg = <0x59810000 0x800>;
			u-boot,dm-pre-reloc;

			mio_clk: clock {
				compatible = "socionext,uniphier-sld3-mio-clock";
				#clock-cells = <1>;
				u-boot,dm-pre-reloc;
			};

			mio_rst: reset {
				compatible = "socionext,uniphier-sld3-mio-reset";
				#reset-cells = <1>;
			};
		};

		emmc: sdhc@5a400000 {
			compatible = "socionext,uniphier-sdhc";
			status = "disabled";
			reg = <0x5a400000 0x200>;
			interrupts = <0 78 4>;
			pinctrl-names = "default", "1.8v";
			pinctrl-0 = <&pinctrl_emmc>;
			pinctrl-1 = <&pinctrl_emmc_1v8>;
			clocks = <&mio_clk 1>;
			reset-names = "host", "bridge";
			resets = <&mio_rst 1>, <&mio_rst 4>;
			bus-width = <8>;
			non-removable;
			cap-mmc-highspeed;
			cap-mmc-hw-reset;
		};

		sd: sdhc@5a500000 {
			compatible = "socionext,uniphier-sdhc";
			status = "disabled";
			reg = <0x5a500000 0x200>;
			interrupts = <0 76 4>;
			pinctrl-names = "default", "1.8v";
			pinctrl-0 = <&pinctrl_sd>;
			pinctrl-1 = <&pinctrl_sd_1v8>;
			clocks = <&mio_clk 0>;
			reset-names = "host", "bridge";
			resets = <&mio_rst 0>, <&mio_rst 3>;
			bus-width = <4>;
			cap-sd-highspeed;
			sd-uhs-sdr12;
			sd-uhs-sdr25;
			sd-uhs-sdr50;
		};

		usb0: usb@5a800100 {
			compatible = "socionext,uniphier-ehci", "generic-ehci";
			status = "disabled";
			reg = <0x5a800100 0x100>;
			interrupts = <0 80 4>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb0>;
			clocks = <&mio_clk 7>, <&mio_clk 8>, <&mio_clk 12>;
			resets = <&sys_rst 8>, <&mio_rst 7>, <&mio_rst 8>,
				 <&mio_rst 12>;
		};

		usb1: usb@5a810100 {
			compatible = "socionext,uniphier-ehci", "generic-ehci";
			status = "disabled";
			reg = <0x5a810100 0x100>;
			interrupts = <0 81 4>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb1>;
			clocks = <&mio_clk 7>, <&mio_clk 9>, <&mio_clk 13>;
			resets = <&sys_rst 8>, <&mio_rst 7>, <&mio_rst 9>,
				 <&mio_rst 13>;
		};

		usb2: usb@5a820100 {
			compatible = "socionext,uniphier-ehci", "generic-ehci";
			status = "disabled";
			reg = <0x5a820100 0x100>;
			interrupts = <0 82 4>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb2>;
			clocks = <&mio_clk 7>, <&mio_clk 10>, <&mio_clk 14>;
			resets = <&sys_rst 8>, <&mio_rst 7>, <&mio_rst 10>,
				 <&mio_rst 14>;
		};

		usb3: usb@5a830100 {
			compatible = "socionext,uniphier-ehci", "generic-ehci";
			status = "disabled";
			reg = <0x5a830100 0x100>;
			interrupts = <0 83 4>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb3>;
			clocks = <&mio_clk 7>, <&mio_clk 11>, <&mio_clk 15>;
			resets = <&sys_rst 8>, <&mio_rst 7>, <&mio_rst 11>,
				 <&mio_rst 15>;
		};

		soc-glue@5f800000 {
			compatible = "socionext,uniphier-sld3-soc-glue",
				     "simple-mfd", "syscon";
			reg = <0x5f800000 0x2000>;
			u-boot,dm-pre-reloc;

			pinctrl: pinctrl {
				compatible = "socionext,uniphier-sld3-pinctrl";
				u-boot,dm-pre-reloc;
			};
		};

		aidet@f1830000 {
			compatible = "simple-mfd", "syscon";
			reg = <0xf1830000 0x200>;
		};

		sysctrl@f1840000 {
			compatible = "socionext,uniphier-sld3-sysctrl",
				     "simple-mfd", "syscon";
			reg = <0xf1840000 0x4000>;

			sys_clk: clock {
				compatible = "socionext,uniphier-sld3-clock";
				#clock-cells = <1>;
			};

			sys_rst: reset {
				compatible = "socionext,uniphier-sld3-reset";
				#reset-cells = <1>;
			};
		};

		nand: nand@f8000000 {
			compatible = "socionext,denali-nand-v5a";
			status = "disabled";
			reg-names = "nand_data", "denali_reg";
			reg = <0xf8000000 0x20>, <0xf8100000 0x1000>;
			interrupts = <0 65 4>;
			clocks = <&sys_clk 2>;
			nand-ecc-strength = <8>;
		};
	};
};

/include/ "uniphier-pinctrl.dtsi"
