/*
 * Device Tree Include file for Marvell Armada XP family SoC
 *
 * Copyright (C) 2012 Marvell
 *
 * Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED , WITHOUT WARRANTY OF ANY KIND
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 *
 * Contains definitions specific to the Armada XP MV78460 SoC that are not
 * common to all Armada XP SoCs.
 */

#include "armada-xp.dtsi"

/ {
	model = "Marvell Armada XP MV78460 SoC";
	compatible = "marvell,armadaxp-mv78460", "marvell,armadaxp", "marvell,armada-370-xp";

	aliases {
		gpio0 = &gpio0;
		gpio1 = &gpio1;
		gpio2 = &gpio2;
	};


	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		enable-method = "marvell,armada-xp-smp";

		cpu@0 {
			device_type = "cpu";
			compatible = "marvell,sheeva-v7";
			reg = <0>;
			clocks = <&cpuclk 0>;
			clock-latency = <1000000>;
		};

		cpu@1 {
			device_type = "cpu";
			compatible = "marvell,sheeva-v7";
			reg = <1>;
			clocks = <&cpuclk 1>;
			clock-latency = <1000000>;
		};

		cpu@2 {
			device_type = "cpu";
			compatible = "marvell,sheeva-v7";
			reg = <2>;
			clocks = <&cpuclk 2>;
			clock-latency = <1000000>;
		};

		cpu@3 {
			device_type = "cpu";
			compatible = "marvell,sheeva-v7";
			reg = <3>;
			clocks = <&cpuclk 3>;
			clock-latency = <1000000>;
		};
	};

	soc {
		/*
		 * MV78460 has 4 PCIe units Gen2.0: Two units can be
		 * configured as x4 or quad x1 lanes. Two units are
		 * x4/x1.
		 */
		pcie-controller {
			compatible = "marvell,armada-xp-pcie";
			status = "disabled";
			device_type = "pci";

			#address-cells = <3>;
			#size-cells = <2>;

			msi-parent = <&mpic>;
			bus-range = <0x00 0xff>;

			ranges =
			       <0x82000000 0 0x40000 MBUS_ID(0xf0, 0x01) 0x40000 0 0x00002000   /* Port 0.0 registers */
				0x82000000 0 0x42000 MBUS_ID(0xf0, 0x01) 0x42000 0 0x00002000   /* Port 2.0 registers */
				0x82000000 0 0x44000 MBUS_ID(0xf0, 0x01) 0x44000 0 0x00002000   /* Port 0.1 registers */
				0x82000000 0 0x48000 MBUS_ID(0xf0, 0x01) 0x48000 0 0x00002000   /* Port 0.2 registers */
				0x82000000 0 0x4c000 MBUS_ID(0xf0, 0x01) 0x4c000 0 0x00002000   /* Port 0.3 registers */
				0x82000000 0 0x80000 MBUS_ID(0xf0, 0x01) 0x80000 0 0x00002000   /* Port 1.0 registers */
				0x82000000 0 0x82000 MBUS_ID(0xf0, 0x01) 0x82000 0 0x00002000   /* Port 3.0 registers */
				0x82000000 0 0x84000 MBUS_ID(0xf0, 0x01) 0x84000 0 0x00002000   /* Port 1.1 registers */
				0x82000000 0 0x88000 MBUS_ID(0xf0, 0x01) 0x88000 0 0x00002000   /* Port 1.2 registers */
				0x82000000 0 0x8c000 MBUS_ID(0xf0, 0x01) 0x8c000 0 0x00002000   /* Port 1.3 registers */
				0x82000000 0x1 0     MBUS_ID(0x04, 0xe8) 0 1 0 /* Port 0.0 MEM */
				0x81000000 0x1 0     MBUS_ID(0x04, 0xe0) 0 1 0 /* Port 0.0 IO  */
				0x82000000 0x2 0     MBUS_ID(0x04, 0xd8) 0 1 0 /* Port 0.1 MEM */
				0x81000000 0x2 0     MBUS_ID(0x04, 0xd0) 0 1 0 /* Port 0.1 IO  */
				0x82000000 0x3 0     MBUS_ID(0x04, 0xb8) 0 1 0 /* Port 0.2 MEM */
				0x81000000 0x3 0     MBUS_ID(0x04, 0xb0) 0 1 0 /* Port 0.2 IO  */
				0x82000000 0x4 0     MBUS_ID(0x04, 0x78) 0 1 0 /* Port 0.3 MEM */
				0x81000000 0x4 0     MBUS_ID(0x04, 0x70) 0 1 0 /* Port 0.3 IO  */

				0x82000000 0x5 0     MBUS_ID(0x08, 0xe8) 0 1 0 /* Port 1.0 MEM */
				0x81000000 0x5 0     MBUS_ID(0x08, 0xe0) 0 1 0 /* Port 1.0 IO  */
				0x82000000 0x6 0     MBUS_ID(0x08, 0xd8) 0 1 0 /* Port 1.1 MEM */
				0x81000000 0x6 0     MBUS_ID(0x08, 0xd0) 0 1 0 /* Port 1.1 IO  */
				0x82000000 0x7 0     MBUS_ID(0x08, 0xb8) 0 1 0 /* Port 1.2 MEM */
				0x81000000 0x7 0     MBUS_ID(0x08, 0xb0) 0 1 0 /* Port 1.2 IO  */
				0x82000000 0x8 0     MBUS_ID(0x08, 0x78) 0 1 0 /* Port 1.3 MEM */
				0x81000000 0x8 0     MBUS_ID(0x08, 0x70) 0 1 0 /* Port 1.3 IO  */

				0x82000000 0x9 0     MBUS_ID(0x04, 0xf8) 0 1 0 /* Port 2.0 MEM */
				0x81000000 0x9 0     MBUS_ID(0x04, 0xf0) 0 1 0 /* Port 2.0 IO  */

				0x82000000 0xa 0     MBUS_ID(0x08, 0xf8) 0 1 0 /* Port 3.0 MEM */
				0x81000000 0xa 0     MBUS_ID(0x08, 0xf0) 0 1 0 /* Port 3.0 IO  */>;

			pcie@1,0 {
				device_type = "pci";
				assigned-addresses = <0x82000800 0 0x40000 0 0x2000>;
				reg = <0x0800 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x1 0 1 0
					  0x81000000 0 0 0x81000000 0x1 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &mpic 58>;
				marvell,pcie-port = <0>;
				marvell,pcie-lane = <0>;
				clocks = <&gateclk 5>;
				status = "disabled";
			};

			pcie@2,0 {
				device_type = "pci";
				assigned-addresses = <0x82001000 0 0x44000 0 0x2000>;
				reg = <0x1000 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x2 0 1 0
					  0x81000000 0 0 0x81000000 0x2 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &mpic 59>;
				marvell,pcie-port = <0>;
				marvell,pcie-lane = <1>;
				clocks = <&gateclk 6>;
				status = "disabled";
			};

			pcie@3,0 {
				device_type = "pci";
				assigned-addresses = <0x82001800 0 0x48000 0 0x2000>;
				reg = <0x1800 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x3 0 1 0
					  0x81000000 0 0 0x81000000 0x3 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &mpic 60>;
				marvell,pcie-port = <0>;
				marvell,pcie-lane = <2>;
				clocks = <&gateclk 7>;
				status = "disabled";
			};

			pcie@4,0 {
				device_type = "pci";
				assigned-addresses = <0x82002000 0 0x4c000 0 0x2000>;
				reg = <0x2000 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x4 0 1 0
					  0x81000000 0 0 0x81000000 0x4 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &mpic 61>;
				marvell,pcie-port = <0>;
				marvell,pcie-lane = <3>;
				clocks = <&gateclk 8>;
				status = "disabled";
			};

			pcie@5,0 {
				device_type = "pci";
				assigned-addresses = <0x82002800 0 0x80000 0 0x2000>;
				reg = <0x2800 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x5 0 1 0
					  0x81000000 0 0 0x81000000 0x5 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &mpic 62>;
				marvell,pcie-port = <1>;
				marvell,pcie-lane = <0>;
				clocks = <&gateclk 9>;
				status = "disabled";
			};

			pcie@6,0 {
				device_type = "pci";
				assigned-addresses = <0x82003000 0 0x84000 0 0x2000>;
				reg = <0x3000 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x6 0 1 0
					  0x81000000 0 0 0x81000000 0x6 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &mpic 63>;
				marvell,pcie-port = <1>;
				marvell,pcie-lane = <1>;
				clocks = <&gateclk 10>;
				status = "disabled";
			};

			pcie@7,0 {
				device_type = "pci";
				assigned-addresses = <0x82003800 0 0x88000 0 0x2000>;
				reg = <0x3800 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x7 0 1 0
					  0x81000000 0 0 0x81000000 0x7 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &mpic 64>;
				marvell,pcie-port = <1>;
				marvell,pcie-lane = <2>;
				clocks = <&gateclk 11>;
				status = "disabled";
			};

			pcie@8,0 {
				device_type = "pci";
				assigned-addresses = <0x82004000 0 0x8c000 0 0x2000>;
				reg = <0x4000 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x8 0 1 0
					  0x81000000 0 0 0x81000000 0x8 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &mpic 65>;
				marvell,pcie-port = <1>;
				marvell,pcie-lane = <3>;
				clocks = <&gateclk 12>;
				status = "disabled";
			};

			pcie@9,0 {
				device_type = "pci";
				assigned-addresses = <0x82004800 0 0x42000 0 0x2000>;
				reg = <0x4800 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0x9 0 1 0
					  0x81000000 0 0 0x81000000 0x9 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &mpic 99>;
				marvell,pcie-port = <2>;
				marvell,pcie-lane = <0>;
				clocks = <&gateclk 26>;
				status = "disabled";
			};

			pcie@10,0 {
				device_type = "pci";
				assigned-addresses = <0x82005000 0 0x82000 0 0x2000>;
				reg = <0x5000 0 0 0 0>;
				#address-cells = <3>;
				#size-cells = <2>;
				#interrupt-cells = <1>;
				ranges = <0x82000000 0 0 0x82000000 0xa 0 1 0
					  0x81000000 0 0 0x81000000 0xa 0 1 0>;
				interrupt-map-mask = <0 0 0 0>;
				interrupt-map = <0 0 0 0 &mpic 103>;
				marvell,pcie-port = <3>;
				marvell,pcie-lane = <0>;
				clocks = <&gateclk 27>;
				status = "disabled";
			};
		};

		internal-regs {
			gpio0: gpio@18100 {
				compatible = "marvell,orion-gpio";
				reg = <0x18100 0x40>;
				ngpios = <32>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <82>, <83>, <84>, <85>;
			};

			gpio1: gpio@18140 {
				compatible = "marvell,orion-gpio";
				reg = <0x18140 0x40>;
				ngpios = <32>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <87>, <88>, <89>, <90>;
			};

			gpio2: gpio@18180 {
				compatible = "marvell,orion-gpio";
				reg = <0x18180 0x40>;
				ngpios = <3>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <91>;
			};

			eth3: ethernet@34000 {
				compatible = "marvell,armada-xp-neta";
				reg = <0x34000 0x4000>;
				interrupts = <14>;
				clocks = <&gateclk 1>;
				status = "disabled";
			};
		};
	};
};

&pinctrl {
	compatible = "marvell,mv78460-pinctrl";
};
