/*
 * Device Tree Include file for Freescale Layerscape-1046A family SoC.
 *
 * Copyright 2016, Freescale Semiconductor
 *
 * Mingkai Hu <Mingkai.hu@freescale.com>
 *
 * This file is licensed under the terms of the GNU General Public
 * License version 2.  This program is licensed "as is" without any
 * warranty of any kind, whether express or implied.
 */

/dts-v1/;
/include/ "fsl-ls1046a.dtsi"

/ {
	model = "LS1046A RDB Board";

	aliases {
		spi0 = &qspi;
	};

};

&qspi {
	bus-num = <0>;
	status = "okay";

	qflash0: s25fs512s@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "spi-flash";
		spi-max-frequency = <50000000>;
		reg = <0>;
	};

	qflash1: s25fs512s@1 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "spi-flash";
		spi-max-frequency = <50000000>;
		reg = <1>;
	 };
};
