/*
 * Copyright 2015 Tyler Baker
 *
 * Tyler Baker <tyler.baker@linaro.org>
 * Chen-Yu Tsai <wens@csie.org>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

/dts-v1/;
#include "sun9i-a80.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/sun4i-a10.h>

/ {
	model = "Cubietech Cubieboard4";
	compatible = "cubietech,a80-cubieboard4", "allwinner,sun9i-a80";

	aliases {
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&led_pins_cubieboard4>;

		green {
			label = "cubieboard4:green:usr";
			gpios = <&pio 7 17 GPIO_ACTIVE_HIGH>; /* PH17 */
		};

		red {
			label = "cubieboard4:red:usr";
			gpios = <&pio 7 6 GPIO_ACTIVE_HIGH>; /* PH6 */
		};
	};
};

&mmc0 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc0_pins>, <&mmc0_cd_pin_cubieboard4>;
	vmmc-supply = <&reg_dcdc1>;
	bus-width = <4>;
	cd-gpios = <&pio 7 18 GPIO_ACTIVE_HIGH>; /* PH18 */
	cd-inverted;
	status = "okay";
};

&mmc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc2_8bit_pins>;
	vmmc-supply = <&reg_dcdc1>;
	bus-width = <8>;
	non-removable;
	cap-mmc-hw-reset;
	status = "okay";
};

&mmc2_8bit_pins {
	/* Increase drive strength for DDR modes */
	allwinner,drive = <SUN4I_PINCTRL_40_MA>;
};

&pio {
	led_pins_cubieboard4: led-pins@0 {
		allwinner,pins = "PH6", "PH17";
		allwinner,function = "gpio_out";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
	};

	mmc0_cd_pin_cubieboard4: mmc0_cd_pin@0 {
		allwinner,pins = "PH18";
		allwinner,function = "gpio_in";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_PULL_UP>;
	};
};

&r_ir {
	status = "okay";
};

&r_rsb {
	status = "okay";

	axp809: pmic@3a3 {
		reg = <0x3a3>;
		interrupt-parent = <&nmi_intc>;
		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;

		regulators {
			reg_aldo1: aldo1 {
				/*
				 * TODO: This should be handled by the
				 * USB PHY driver.
				 */
				regulator-always-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc33-usbh";
			};

			reg_aldo2: aldo2 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc-pb-io-cam";
			};

			aldo3 {
				/* unused */
			};

			reg_dc5ldo: dc5ldo {
				regulator-always-on;
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1100000>;
				regulator-name = "vdd-cpus-09-usbh";
			};

			reg_dcdc1: dcdc1 {
				regulator-always-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc-3v";
			};

			reg_dcdc2: dcdc2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1100000>;
				regulator-name = "vdd-gpu";
			};

			reg_dcdc3: dcdc3 {
				regulator-always-on;
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1100000>;
				regulator-name = "vdd-cpua";
			};

			reg_dcdc4: dcdc4 {
				regulator-always-on;
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1100000>;
				regulator-name = "vdd-sys-usb0-hdmi";
			};

			reg_dcdc5: dcdc5 {
				regulator-always-on;
				regulator-min-microvolt = <1425000>;
				regulator-max-microvolt = <1575000>;
				regulator-name = "vcc-dram";
			};

			reg_dldo1: dldo1 {
				/*
				 * The WiFi chip supports a wide range
				 * (3.0 ~ 4.8V) of voltages, and so does
				 * this regulator (3.0 ~ 4.2V), but
				 * Allwinner SDK always sets it to 3.3V.
				 */
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc-wifi";
			};

			reg_dldo2: dldo2 {
				regulator-always-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc-pl";
			};

			reg_eldo1: eldo1 {
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
				regulator-name = "vcc-dvdd-cam";
			};

			reg_eldo2: eldo2 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc-pe";
			};

			reg_eldo3: eldo3 {
				regulator-always-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc-pm-codec-io1";
			};

			reg_ldo_io0: ldo_io0 {
				regulator-always-on;
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-name = "vcc-pg";
			};

			reg_ldo_io1: ldo_io1 {
				regulator-min-microvolt = <2500000>;
				regulator-max-microvolt = <2500000>;
				regulator-name = "vcc-pa-gmac-2v5";
			};

			reg_rtc_ldo: rtc_ldo {
				regulator-name = "vcc-rtc-vdd1v8-io";
			};
		};
	};
};

#include "axp809.dtsi"

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pins_a>;
	status = "okay";
};
