/*
 * at91sam9g45.dtsi - Device Tree Include file for AT91SAM9G45 family SoC
 *                    applies to AT91SAM9G45, AT91SAM9M10,
 *                    AT91SAM9G46, AT91SAM9M11 SoC
 *
 *  Copyright (C) 2011 Atmel,
 *                2011 Nicolas Ferre <nicolas.ferre@atmel.com>
 *
 * Licensed under GPLv2 or later.
 */

#include "skeleton.dtsi"
#include <dt-bindings/dma/at91.h>
#include <dt-bindings/pinctrl/at91.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/clock/at91.h>

/ {
	model = "Atmel AT91SAM9G45 family SoC";
	compatible = "atmel,at91sam9g45";
	interrupt-parent = <&aic>;

	aliases {
		serial0 = &dbgu;
		serial1 = &usart0;
		serial2 = &usart1;
		serial3 = &usart2;
		serial4 = &usart3;
		gpio0 = &pioA;
		gpio1 = &pioB;
		gpio2 = &pioC;
		gpio3 = &pioD;
		gpio4 = &pioE;
		tcb0 = &tcb0;
		tcb1 = &tcb1;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		ssc0 = &ssc0;
		ssc1 = &ssc1;
		pwm0 = &pwm0;
	};
	cpus {
		#address-cells = <0>;
		#size-cells = <0>;

		cpu {
			compatible = "arm,arm926ej-s";
			device_type = "cpu";
		};
	};

	memory {
		reg = <0x70000000 0x10000000>;
	};

	clocks {
		slow_xtal: slow_xtal {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};

		main_xtal: main_xtal {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};

		adc_op_clk: adc_op_clk{
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <300000>;
		};
	};

	sram: sram@00300000 {
		compatible = "mmio-sram";
		reg = <0x00300000 0x10000>;
	};

	ahb {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		apb {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			aic: interrupt-controller@fffff000 {
				#interrupt-cells = <3>;
				compatible = "atmel,at91rm9200-aic";
				interrupt-controller;
				reg = <0xfffff000 0x200>;
				atmel,external-irqs = <31>;
			};

			ramc0: ramc@ffffe400 {
				compatible = "atmel,at91sam9g45-ddramc";
				reg = <0xffffe400 0x200>;
				clocks = <&ddrck>;
				clock-names = "ddrck";
			};

			ramc1: ramc@ffffe600 {
				compatible = "atmel,at91sam9g45-ddramc";
				reg = <0xffffe600 0x200>;
				clocks = <&ddrck>;
				clock-names = "ddrck";
			};

			pmc: pmc@fffffc00 {
				compatible = "atmel,at91sam9g45-pmc", "syscon";
				reg = <0xfffffc00 0x100>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				interrupt-controller;
				#address-cells = <1>;
				#size-cells = <0>;
				#interrupt-cells = <1>;

				main_osc: main_osc {
					compatible = "atmel,at91rm9200-clk-main-osc";
					#clock-cells = <0>;
					interrupts-extended = <&pmc AT91_PMC_MOSCS>;
					clocks = <&main_xtal>;
				};

				main: mainck {
					compatible = "atmel,at91rm9200-clk-main";
					#clock-cells = <0>;
					clocks = <&main_osc>;
				};

				plla: pllack {
					compatible = "atmel,at91rm9200-clk-pll";
					#clock-cells = <0>;
					interrupts-extended = <&pmc AT91_PMC_LOCKA>;
					clocks = <&main>;
					reg = <0>;
					atmel,clk-input-range = <2000000 32000000>;
					#atmel,pll-clk-output-range-cells = <4>;
					atmel,pll-clk-output-ranges = <745000000 800000000 0 0
								       695000000 750000000 1 0
								       645000000 700000000 2 0
								       595000000 650000000 3 0
								       545000000 600000000 0 1
								       495000000 555000000 1 1
								       445000000 500000000 2 1
								       400000000 450000000 3 1>;
				};

				plladiv: plladivck {
					compatible = "atmel,at91sam9x5-clk-plldiv";
					#clock-cells = <0>;
					clocks = <&plla>;
				};

				utmi: utmick {
					compatible = "atmel,at91sam9x5-clk-utmi";
					#clock-cells = <0>;
					interrupts-extended = <&pmc AT91_PMC_LOCKU>;
					clocks = <&main>;
				};

				mck: masterck {
					compatible = "atmel,at91rm9200-clk-master";
					#clock-cells = <0>;
					interrupts-extended = <&pmc AT91_PMC_MCKRDY>;
					clocks = <&clk32k>, <&main>, <&plladiv>, <&utmi>;
					atmel,clk-output-range = <0 133333333>;
					atmel,clk-divisors = <1 2 4 3>;
				};

				usb: usbck {
					compatible = "atmel,at91sam9x5-clk-usb";
					#clock-cells = <0>;
					clocks = <&plladiv>, <&utmi>;
				};

				prog: progck {
					compatible = "atmel,at91sam9g45-clk-programmable";
					#address-cells = <1>;
					#size-cells = <0>;
					interrupt-parent = <&pmc>;
					clocks = <&clk32k>, <&main>, <&plladiv>, <&utmi>, <&mck>;

					prog0: prog0 {
						#clock-cells = <0>;
						reg = <0>;
						interrupts = <AT91_PMC_PCKRDY(0)>;
					};

					prog1: prog1 {
						#clock-cells = <0>;
						reg = <1>;
						interrupts = <AT91_PMC_PCKRDY(1)>;
					};
				};

				systemck {
					compatible = "atmel,at91rm9200-clk-system";
					#address-cells = <1>;
					#size-cells = <0>;

					ddrck: ddrck {
						#clock-cells = <0>;
						reg = <2>;
						clocks = <&mck>;
					};

					uhpck: uhpck {
						#clock-cells = <0>;
						reg = <6>;
						clocks = <&usb>;
					};

					pck0: pck0 {
						#clock-cells = <0>;
						reg = <8>;
						clocks = <&prog0>;
					};

					pck1: pck1 {
						#clock-cells = <0>;
						reg = <9>;
						clocks = <&prog1>;
					};
				};

				periphck {
					compatible = "atmel,at91rm9200-clk-peripheral";
					#address-cells = <1>;
					#size-cells = <0>;
					clocks = <&mck>;

					pioA_clk: pioA_clk {
						#clock-cells = <0>;
						reg = <2>;
					};

					pioB_clk: pioB_clk {
						#clock-cells = <0>;
						reg = <3>;
					};

					pioC_clk: pioC_clk {
						#clock-cells = <0>;
						reg = <4>;
					};

					pioDE_clk: pioDE_clk {
						#clock-cells = <0>;
						reg = <5>;
					};

					trng_clk: trng_clk {
						#clock-cells = <0>;
						reg = <6>;
					};

					usart0_clk: usart0_clk {
						#clock-cells = <0>;
						reg = <7>;
					};

					usart1_clk: usart1_clk {
						#clock-cells = <0>;
						reg = <8>;
					};

					usart2_clk: usart2_clk {
						#clock-cells = <0>;
						reg = <9>;
					};

					usart3_clk: usart3_clk {
						#clock-cells = <0>;
						reg = <10>;
					};

					mci0_clk: mci0_clk {
						#clock-cells = <0>;
						reg = <11>;
					};

					twi0_clk: twi0_clk {
						#clock-cells = <0>;
						reg = <12>;
					};

					twi1_clk: twi1_clk {
						#clock-cells = <0>;
						reg = <13>;
					};

					spi0_clk: spi0_clk {
						#clock-cells = <0>;
						reg = <14>;
					};

					spi1_clk: spi1_clk {
						#clock-cells = <0>;
						reg = <15>;
					};

					ssc0_clk: ssc0_clk {
						#clock-cells = <0>;
						reg = <16>;
					};

					ssc1_clk: ssc1_clk {
						#clock-cells = <0>;
						reg = <17>;
					};

					tcb0_clk: tcb0_clk {
						#clock-cells = <0>;
						reg = <18>;
					};

					pwm_clk: pwm_clk {
						#clock-cells = <0>;
						reg = <19>;
					};

					adc_clk: adc_clk {
						#clock-cells = <0>;
						reg = <20>;
					};

					dma0_clk: dma0_clk {
						#clock-cells = <0>;
						reg = <21>;
					};

					uhphs_clk: uhphs_clk {
						#clock-cells = <0>;
						reg = <22>;
					};

					lcd_clk: lcd_clk {
						#clock-cells = <0>;
						reg = <23>;
					};

					ac97_clk: ac97_clk {
						#clock-cells = <0>;
						reg = <24>;
					};

					macb0_clk: macb0_clk {
						#clock-cells = <0>;
						reg = <25>;
					};

					isi_clk: isi_clk {
						#clock-cells = <0>;
						reg = <26>;
					};

					udphs_clk: udphs_clk {
						#clock-cells = <0>;
						reg = <27>;
					};

					aestdessha_clk: aestdessha_clk {
						#clock-cells = <0>;
						reg = <28>;
					};

					mci1_clk: mci1_clk {
						#clock-cells = <0>;
						reg = <29>;
					};

					vdec_clk: vdec_clk {
						#clock-cells = <0>;
						reg = <30>;
					};
				};
			};

			rstc@fffffd00 {
				compatible = "atmel,at91sam9g45-rstc";
				reg = <0xfffffd00 0x10>;
				clocks = <&clk32k>;
			};

			pit: timer@fffffd30 {
				compatible = "atmel,at91sam9260-pit";
				reg = <0xfffffd30 0xf>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				clocks = <&mck>;
			};


			shdwc@fffffd10 {
				compatible = "atmel,at91sam9rl-shdwc";
				reg = <0xfffffd10 0x10>;
				clocks = <&clk32k>;
			};

			tcb0: timer@fff7c000 {
				compatible = "atmel,at91rm9200-tcb";
				reg = <0xfff7c000 0x100>;
				interrupts = <18 IRQ_TYPE_LEVEL_HIGH 0>;
				clocks = <&tcb0_clk>, <&tcb0_clk>, <&tcb0_clk>, <&clk32k>;
				clock-names = "t0_clk", "t1_clk", "t2_clk", "slow_clk";
			};

			tcb1: timer@fffd4000 {
				compatible = "atmel,at91rm9200-tcb";
				reg = <0xfffd4000 0x100>;
				interrupts = <18 IRQ_TYPE_LEVEL_HIGH 0>;
				clocks = <&tcb0_clk>, <&tcb0_clk>, <&tcb0_clk>, <&clk32k>;
				clock-names = "t0_clk", "t1_clk", "t2_clk", "slow_clk";
			};

			dma: dma-controller@ffffec00 {
				compatible = "atmel,at91sam9g45-dma";
				reg = <0xffffec00 0x200>;
				interrupts = <21 IRQ_TYPE_LEVEL_HIGH 0>;
				#dma-cells = <2>;
				clocks = <&dma0_clk>;
				clock-names = "dma_clk";
			};

			pinctrl@fffff200 {
				#address-cells = <1>;
				#size-cells = <1>;
				compatible = "atmel,at91rm9200-pinctrl", "simple-bus";
				ranges = <0xfffff200 0xfffff200 0xa00>;

				atmel,mux-mask = <
				      /*    A         B     */
				       0xffffffff 0xffc003ff  /* pioA */
				       0xffffffff 0x800f8f00  /* pioB */
				       0xffffffff 0x00000e00  /* pioC */
				       0xffffffff 0xff0c1381  /* pioD */
				       0xffffffff 0x81ffff81  /* pioE */
				      >;

				/* shared pinctrl settings */
				adc0 {
					pinctrl_adc0_adtrg: adc0_adtrg {
						atmel,pins = <AT91_PIOD 28 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};
					pinctrl_adc0_ad0: adc0_ad0 {
						atmel,pins = <AT91_PIOD 20 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
					pinctrl_adc0_ad1: adc0_ad1 {
						atmel,pins = <AT91_PIOD 21 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
					pinctrl_adc0_ad2: adc0_ad2 {
						atmel,pins = <AT91_PIOD 22 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
					pinctrl_adc0_ad3: adc0_ad3 {
						atmel,pins = <AT91_PIOD 23 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
					pinctrl_adc0_ad4: adc0_ad4 {
						atmel,pins = <AT91_PIOD 24 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
					pinctrl_adc0_ad5: adc0_ad5 {
						atmel,pins = <AT91_PIOD 25 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
					pinctrl_adc0_ad6: adc0_ad6 {
						atmel,pins = <AT91_PIOD 26 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
					pinctrl_adc0_ad7: adc0_ad7 {
						atmel,pins = <AT91_PIOD 27 AT91_PERIPH_GPIO AT91_PINCTRL_NONE>;
					};
				};

				dbgu {
					pinctrl_dbgu: dbgu-0 {
						atmel,pins =
							<AT91_PIOB 12 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB12 periph A */
							 AT91_PIOB 13 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB13 periph A */
					};
				};

				i2c0 {
					pinctrl_i2c0: i2c0-0 {
						atmel,pins =
							<AT91_PIOA 21 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA21 periph A TWCK0 */
							 AT91_PIOA 20 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA20 periph A TWD0 */
					};
				};

				i2c1 {
					pinctrl_i2c1: i2c1-0 {
						atmel,pins =
							<AT91_PIOB 11 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB11 periph A TWCK1 */
							 AT91_PIOB 10 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB10 periph A TWD1 */
					};
				};

				isi {
					pinctrl_isi_data_0_7: isi-0-data-0-7 {
						atmel,pins =
							<AT91_PIOB 20 AT91_PERIPH_A AT91_PINCTRL_NONE /* D0 */
							AT91_PIOB 21 AT91_PERIPH_A AT91_PINCTRL_NONE /* D1 */
							AT91_PIOB 22 AT91_PERIPH_A AT91_PINCTRL_NONE /* D2 */
							AT91_PIOB 23 AT91_PERIPH_A AT91_PINCTRL_NONE /* D3 */
							AT91_PIOB 24 AT91_PERIPH_A AT91_PINCTRL_NONE /* D4 */
							AT91_PIOB 25 AT91_PERIPH_A AT91_PINCTRL_NONE /* D5 */
							AT91_PIOB 26 AT91_PERIPH_A AT91_PINCTRL_NONE /* D6 */
							AT91_PIOB 27 AT91_PERIPH_A AT91_PINCTRL_NONE /* D7 */
							AT91_PIOB 28 AT91_PERIPH_A AT91_PINCTRL_NONE /* PCK */
							AT91_PIOB 29 AT91_PERIPH_A AT91_PINCTRL_NONE /* VSYNC */
							AT91_PIOB 30 AT91_PERIPH_A AT91_PINCTRL_NONE>; /* HSYNC */
					};

					pinctrl_isi_data_8_9: isi-0-data-8-9 {
						atmel,pins =
							<AT91_PIOB 8 AT91_PERIPH_B AT91_PINCTRL_NONE /* D8 */
							AT91_PIOB 9 AT91_PERIPH_B AT91_PINCTRL_NONE>; /* D9 */
					};

					pinctrl_isi_data_10_11: isi-0-data-10-11 {
						atmel,pins =
							<AT91_PIOB 10 AT91_PERIPH_B AT91_PINCTRL_NONE /* D10 */
							AT91_PIOB 11 AT91_PERIPH_B AT91_PINCTRL_NONE>; /* D11 */
					};
				};

				usart0 {
					pinctrl_usart0: usart0-0 {
						atmel,pins =
							<AT91_PIOB 19 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PB19 periph A with pullup */
							 AT91_PIOB 18 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB18 periph A */
					};

					pinctrl_usart0_rts: usart0_rts-0 {
						atmel,pins =
							<AT91_PIOB 17 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PB17 periph B */
					};

					pinctrl_usart0_cts: usart0_cts-0 {
						atmel,pins =
							<AT91_PIOB 15 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PB15 periph B */
					};
				};

				uart1 {
					pinctrl_usart1: usart1-0 {
						atmel,pins =
							<AT91_PIOB 4 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PB4 periph A with pullup */
							 AT91_PIOB 5 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB5 periph A */
					};

					pinctrl_usart1_rts: usart1_rts-0 {
						atmel,pins =
							<AT91_PIOD 16 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD16 periph A */
					};

					pinctrl_usart1_cts: usart1_cts-0 {
						atmel,pins =
							<AT91_PIOD 17 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD17 periph A */
					};
				};

				usart2 {
					pinctrl_usart2: usart2-0 {
						atmel,pins =
							<AT91_PIOB 6 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PB6 periph A with pullup */
							 AT91_PIOB 7 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB7 periph A */
					};

					pinctrl_usart2_rts: usart2_rts-0 {
						atmel,pins =
							<AT91_PIOC 9 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PC9 periph B */
					};

					pinctrl_usart2_cts: usart2_cts-0 {
						atmel,pins =
							<AT91_PIOC 11 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PC11 periph B */
					};
				};

				usart3 {
					pinctrl_usart3: usart3-0 {
						atmel,pins =
							<AT91_PIOB 8 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PB9 periph A with pullup */
							 AT91_PIOB 9 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB8 periph A */
					};

					pinctrl_usart3_rts: usart3_rts-0 {
						atmel,pins =
							<AT91_PIOA 23 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PA23 periph B */
					};

					pinctrl_usart3_cts: usart3_cts-0 {
						atmel,pins =
							<AT91_PIOA 24 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PA24 periph B */
					};
				};

				nand {
					pinctrl_nand: nand-0 {
						atmel,pins =
							<AT91_PIOC 8 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP	/* PC8 gpio RDY pin pull_up*/
							 AT91_PIOC 14 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP>;	/* PC14 gpio enable pin pull_up */
					};
				};

				macb {
					pinctrl_macb_rmii: macb_rmii-0 {
						atmel,pins =
							<AT91_PIOA 10 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA10 periph A */
							 AT91_PIOA 11 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA11 periph A */
							 AT91_PIOA 12 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA12 periph A */
							 AT91_PIOA 13 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA13 periph A */
							 AT91_PIOA 14 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA14 periph A */
							 AT91_PIOA 15 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA15 periph A */
							 AT91_PIOA 16 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA16 periph A */
							 AT91_PIOA 17 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA17 periph A */
							 AT91_PIOA 18 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA18 periph A */
							 AT91_PIOA 19 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA19 periph A */
					};

					pinctrl_macb_rmii_mii: macb_rmii_mii-0 {
						atmel,pins =
							<AT91_PIOA 6 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA6 periph B */
							 AT91_PIOA 7 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA7 periph B */
							 AT91_PIOA 8 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA8 periph B */
							 AT91_PIOA 9 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA9 periph B */
							 AT91_PIOA 27 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA27 periph B */
							 AT91_PIOA 28 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA28 periph B */
							 AT91_PIOA 29 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA29 periph B */
							 AT91_PIOA 30 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PA30 periph B */
					};
				};

				mmc0 {
					pinctrl_mmc0_slot0_clk_cmd_dat0: mmc0_slot0_clk_cmd_dat0-0 {
						atmel,pins =
							<AT91_PIOA 0 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA0 periph A */
							 AT91_PIOA 1 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA1 periph A with pullup */
							 AT91_PIOA 2 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA2 periph A with pullup */
					};

					pinctrl_mmc0_slot0_dat1_3: mmc0_slot0_dat1_3-0 {
						atmel,pins =
							<AT91_PIOA 3 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA3 periph A with pullup */
							 AT91_PIOA 4 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA4 periph A with pullup */
							 AT91_PIOA 5 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA5 periph A with pullup */
					};

					pinctrl_mmc0_slot0_dat4_7: mmc0_slot0_dat4_7-0 {
						atmel,pins =
							<AT91_PIOA 6 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA6 periph A with pullup */
							 AT91_PIOA 7 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA7 periph A with pullup */
							 AT91_PIOA 8 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA8 periph A with pullup */
							 AT91_PIOA 9 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA9 periph A with pullup */
					};
				};

				mmc1 {
					pinctrl_mmc1_slot0_clk_cmd_dat0: mmc1_slot0_clk_cmd_dat0-0 {
						atmel,pins =
							<AT91_PIOA 31 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA31 periph A */
							 AT91_PIOA 22 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA22 periph A with pullup */
							 AT91_PIOA 23 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA23 periph A with pullup */
					};

					pinctrl_mmc1_slot0_dat1_3: mmc1_slot0_dat1_3-0 {
						atmel,pins =
							<AT91_PIOA 24 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA24 periph A with pullup */
							 AT91_PIOA 25 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA25 periph A with pullup */
							 AT91_PIOA 26 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA26 periph A with pullup */
					};

					pinctrl_mmc1_slot0_dat4_7: mmc1_slot0_dat4_7-0 {
						atmel,pins =
							<AT91_PIOA 27 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA27 periph A with pullup */
							 AT91_PIOA 28 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA28 periph A with pullup */
							 AT91_PIOA 29 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA29 periph A with pullup */
							 AT91_PIOA 20 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA30 periph A with pullup */
					};
				};

				ssc0 {
					pinctrl_ssc0_tx: ssc0_tx-0 {
						atmel,pins =
							<AT91_PIOD 0 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD0 periph A */
							 AT91_PIOD 1 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD1 periph A */
							 AT91_PIOD 2 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD2 periph A */
					};

					pinctrl_ssc0_rx: ssc0_rx-0 {
						atmel,pins =
							<AT91_PIOD 3 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD3 periph A */
							 AT91_PIOD 4 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD4 periph A */
							 AT91_PIOD 5 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD5 periph A */
					};
				};

				ssc1 {
					pinctrl_ssc1_tx: ssc1_tx-0 {
						atmel,pins =
							<AT91_PIOD 10 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD10 periph A */
							 AT91_PIOD 11 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD11 periph A */
							 AT91_PIOD 12 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD12 periph A */
					};

					pinctrl_ssc1_rx: ssc1_rx-0 {
						atmel,pins =
							<AT91_PIOD 13 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD13 periph A */
							 AT91_PIOD 14 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD14 periph A */
							 AT91_PIOD 15 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD15 periph A */
					};
				};

				spi0 {
					pinctrl_spi0: spi0-0 {
						atmel,pins =
							<AT91_PIOB 0 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB0 periph A SPI0_MISO pin */
							 AT91_PIOB 1 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB1 periph A SPI0_MOSI pin */
							 AT91_PIOB 2 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB2 periph A SPI0_SPCK pin */
					};
				};

				spi1 {
					pinctrl_spi1: spi1-0 {
						atmel,pins =
							<AT91_PIOB 14 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB14 periph A SPI1_MISO pin */
							 AT91_PIOB 15 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PB15 periph A SPI1_MOSI pin */
							 AT91_PIOB 16 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PB16 periph A SPI1_SPCK pin */
					};
				};

				tcb0 {
					pinctrl_tcb0_tclk0: tcb0_tclk0-0 {
						atmel,pins = <AT91_PIOD 23 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tclk1: tcb0_tclk1-0 {
						atmel,pins = <AT91_PIOD 29 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tclk2: tcb0_tclk2-0 {
						atmel,pins = <AT91_PIOC 10 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tioa0: tcb0_tioa0-0 {
						atmel,pins = <AT91_PIOD 20 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tioa1: tcb0_tioa1-0 {
						atmel,pins = <AT91_PIOD 21 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tioa2: tcb0_tioa2-0 {
						atmel,pins = <AT91_PIOD 22 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tiob0: tcb0_tiob0-0 {
						atmel,pins = <AT91_PIOD 30 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tiob1: tcb0_tiob1-0 {
						atmel,pins = <AT91_PIOD 31 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tiob2: tcb0_tiob2-0 {
						atmel,pins = <AT91_PIOA 26 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};
				};

				tcb1 {
					pinctrl_tcb1_tclk0: tcb1_tclk0-0 {
						atmel,pins = <AT91_PIOA 0 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tclk1: tcb1_tclk1-0 {
						atmel,pins = <AT91_PIOA 3 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tclk2: tcb1_tclk2-0 {
						atmel,pins = <AT91_PIOD 9 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tioa0: tcb1_tioa0-0 {
						atmel,pins = <AT91_PIOA 1 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tioa1: tcb1_tioa1-0 {
						atmel,pins = <AT91_PIOA 4 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tioa2: tcb1_tioa2-0 {
						atmel,pins = <AT91_PIOD 7 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tiob0: tcb1_tiob0-0 {
						atmel,pins = <AT91_PIOA 2 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tiob1: tcb1_tiob1-0 {
						atmel,pins = <AT91_PIOA 5 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tiob2: tcb1_tiob2-0 {
						atmel,pins = <AT91_PIOD 8 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};
				};

				fb {
					pinctrl_fb: fb-0 {
						atmel,pins =
							<AT91_PIOE 0 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE0 periph A */
							 AT91_PIOE 2 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE2 periph A */
							 AT91_PIOE 3 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE3 periph A */
							 AT91_PIOE 4 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE4 periph A */
							 AT91_PIOE 5 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE5 periph A */
							 AT91_PIOE 6 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE6 periph A */
							 AT91_PIOE 7 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE7 periph A */
							 AT91_PIOE 8 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE8 periph A */
							 AT91_PIOE 9 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE9 periph A */
							 AT91_PIOE 10 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE10 periph A */
							 AT91_PIOE 11 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE11 periph A */
							 AT91_PIOE 12 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE12 periph A */
							 AT91_PIOE 13 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE13 periph A */
							 AT91_PIOE 14 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE14 periph A */
							 AT91_PIOE 15 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE15 periph A */
							 AT91_PIOE 16 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE16 periph A */
							 AT91_PIOE 17 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE17 periph A */
							 AT91_PIOE 18 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE18 periph A */
							 AT91_PIOE 19 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE19 periph A */
							 AT91_PIOE 20 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE20 periph A */
							 AT91_PIOE 21 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE21 periph A */
							 AT91_PIOE 22 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE22 periph A */
							 AT91_PIOE 23 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE23 periph A */
							 AT91_PIOE 24 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE24 periph A */
							 AT91_PIOE 25 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE25 periph A */
							 AT91_PIOE 26 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE26 periph A */
							 AT91_PIOE 27 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE27 periph A */
							 AT91_PIOE 28 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE28 periph A */
							 AT91_PIOE 29 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PE29 periph A */
							 AT91_PIOE 30 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PE30 periph A */
					};
				};

				pioA: gpio@fffff200 {
					compatible = "atmel,at91rm9200-gpio";
					reg = <0xfffff200 0x200>;
					interrupts = <2 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioA_clk>;
				};

				pioB: gpio@fffff400 {
					compatible = "atmel,at91rm9200-gpio";
					reg = <0xfffff400 0x200>;
					interrupts = <3 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioB_clk>;
				};

				pioC: gpio@fffff600 {
					compatible = "atmel,at91rm9200-gpio";
					reg = <0xfffff600 0x200>;
					interrupts = <4 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioC_clk>;
				};

				pioD: gpio@fffff800 {
					compatible = "atmel,at91rm9200-gpio";
					reg = <0xfffff800 0x200>;
					interrupts = <5 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioDE_clk>;
				};

				pioE: gpio@fffffa00 {
					compatible = "atmel,at91rm9200-gpio";
					reg = <0xfffffa00 0x200>;
					interrupts = <5 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
					clocks = <&pioDE_clk>;
				};
			};

			dbgu: serial@ffffee00 {
				compatible = "atmel,at91sam9260-dbgu", "atmel,at91sam9260-usart";
				reg = <0xffffee00 0x200>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_dbgu>;
				clocks = <&mck>;
				clock-names = "usart";
				status = "disabled";
			};

			usart0: serial@fff8c000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xfff8c000 0x200>;
				interrupts = <7 IRQ_TYPE_LEVEL_HIGH 5>;
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart0>;
				clocks = <&usart0_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			usart1: serial@fff90000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xfff90000 0x200>;
				interrupts = <8 IRQ_TYPE_LEVEL_HIGH 5>;
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart1>;
				clocks = <&usart1_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			usart2: serial@fff94000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xfff94000 0x200>;
				interrupts = <9 IRQ_TYPE_LEVEL_HIGH 5>;
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart2>;
				clocks = <&usart2_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			usart3: serial@fff98000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xfff98000 0x200>;
				interrupts = <10 IRQ_TYPE_LEVEL_HIGH 5>;
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart3>;
				clocks = <&usart3_clk>;
				clock-names = "usart";
				status = "disabled";
			};

			macb0: ethernet@fffbc000 {
				compatible = "cdns,at91sam9260-macb", "cdns,macb";
				reg = <0xfffbc000 0x100>;
				interrupts = <25 IRQ_TYPE_LEVEL_HIGH 3>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_macb_rmii>;
				clocks = <&macb0_clk>, <&macb0_clk>;
				clock-names = "hclk", "pclk";
				status = "disabled";
			};

			trng@fffcc000 {
				compatible = "atmel,at91sam9g45-trng";
				reg = <0xfffcc000 0x4000>;
				interrupts = <6 IRQ_TYPE_LEVEL_HIGH 0>;
				clocks = <&trng_clk>;
			};

			i2c0: i2c@fff84000 {
				compatible = "atmel,at91sam9g10-i2c";
				reg = <0xfff84000 0x100>;
				interrupts = <12 IRQ_TYPE_LEVEL_HIGH 6>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_i2c0>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&twi0_clk>;
				status = "disabled";
			};

			i2c1: i2c@fff88000 {
				compatible = "atmel,at91sam9g10-i2c";
				reg = <0xfff88000 0x100>;
				interrupts = <13 IRQ_TYPE_LEVEL_HIGH 6>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_i2c1>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&twi1_clk>;
				status = "disabled";
			};

			ssc0: ssc@fff9c000 {
				compatible = "atmel,at91sam9g45-ssc";
				reg = <0xfff9c000 0x4000>;
				interrupts = <16 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_ssc0_tx &pinctrl_ssc0_rx>;
				clocks = <&ssc0_clk>;
				clock-names = "pclk";
				status = "disabled";
			};

			ssc1: ssc@fffa0000 {
				compatible = "atmel,at91sam9g45-ssc";
				reg = <0xfffa0000 0x4000>;
				interrupts = <17 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_ssc1_tx &pinctrl_ssc1_rx>;
				clocks = <&ssc1_clk>;
				clock-names = "pclk";
				status = "disabled";
			};

			adc0: adc@fffb0000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91sam9g45-adc";
				reg = <0xfffb0000 0x100>;
				interrupts = <20 IRQ_TYPE_LEVEL_HIGH 0>;
				clocks = <&adc_clk>, <&adc_op_clk>;
				clock-names = "adc_clk", "adc_op_clk";
				atmel,adc-channels-used = <0xff>;
				atmel,adc-vref = <3300>;
				atmel,adc-startup-time = <40>;
				atmel,adc-res = <8 10>;
				atmel,adc-res-names = "lowres", "highres";
				atmel,adc-use-res = "highres";

				trigger@0 {
					reg = <0>;
					trigger-name = "external-rising";
					trigger-value = <0x1>;
					trigger-external;
				};
				trigger@1 {
					reg = <1>;
					trigger-name = "external-falling";
					trigger-value = <0x2>;
					trigger-external;
				};

				trigger@2 {
					reg = <2>;
					trigger-name = "external-any";
					trigger-value = <0x3>;
					trigger-external;
				};

				trigger@3 {
					reg = <3>;
					trigger-name = "continuous";
					trigger-value = <0x6>;
				};
			};

			isi@fffb4000 {
				compatible = "atmel,at91sam9g45-isi";
				reg = <0xfffb4000 0x4000>;
				interrupts = <26 IRQ_TYPE_LEVEL_HIGH 5>;
				clocks = <&isi_clk>;
				clock-names = "isi_clk";
				status = "disabled";
				port {
					#address-cells = <1>;
					#size-cells = <0>;
				};
			};

			pwm0: pwm@fffb8000 {
				compatible = "atmel,at91sam9rl-pwm";
				reg = <0xfffb8000 0x300>;
				interrupts = <19 IRQ_TYPE_LEVEL_HIGH 4>;
				#pwm-cells = <3>;
				clocks = <&pwm_clk>;
				status = "disabled";
			};

			mmc0: mmc@fff80000 {
				compatible = "atmel,hsmci";
				reg = <0xfff80000 0x600>;
				interrupts = <11 IRQ_TYPE_LEVEL_HIGH 0>;
				pinctrl-names = "default";
				dmas = <&dma 1 AT91_DMA_CFG_PER_ID(0)>;
				dma-names = "rxtx";
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&mci0_clk>;
				clock-names = "mci_clk";
				status = "disabled";
			};

			mmc1: mmc@fffd0000 {
				compatible = "atmel,hsmci";
				reg = <0xfffd0000 0x600>;
				interrupts = <29 IRQ_TYPE_LEVEL_HIGH 0>;
				pinctrl-names = "default";
				dmas = <&dma 1 AT91_DMA_CFG_PER_ID(13)>;
				dma-names = "rxtx";
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&mci1_clk>;
				clock-names = "mci_clk";
				status = "disabled";
			};

			watchdog@fffffd40 {
				compatible = "atmel,at91sam9260-wdt";
				reg = <0xfffffd40 0x10>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				clocks = <&clk32k>;
				atmel,watchdog-type = "hardware";
				atmel,reset-type = "all";
				atmel,dbg-halt;
				status = "disabled";
			};

			spi0: spi@fffa4000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91rm9200-spi";
				reg = <0xfffa4000 0x200>;
				interrupts = <14 4 3>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_spi0>;
				clocks = <&spi0_clk>;
				clock-names = "spi_clk";
				status = "disabled";
			};

			spi1: spi@fffa8000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91rm9200-spi";
				reg = <0xfffa8000 0x200>;
				interrupts = <15 4 3>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_spi1>;
				clocks = <&spi1_clk>;
				clock-names = "spi_clk";
				status = "disabled";
			};

			usb2: gadget@fff78000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91sam9g45-udc";
				reg = <0x00600000 0x80000
				       0xfff78000 0x400>;
				interrupts = <27 IRQ_TYPE_LEVEL_HIGH 0>;
				clocks = <&udphs_clk>, <&utmi>;
				clock-names = "pclk", "hclk";
				status = "disabled";

				ep0 {
					reg = <0>;
					atmel,fifo-size = <64>;
					atmel,nb-banks = <1>;
				};

				ep1 {
					reg = <1>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <2>;
					atmel,can-dma;
					atmel,can-isoc;
				};

				ep2 {
					reg = <2>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <2>;
					atmel,can-dma;
					atmel,can-isoc;
				};

				ep3 {
					reg = <3>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <3>;
					atmel,can-dma;
				};

				ep4 {
					reg = <4>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <3>;
					atmel,can-dma;
				};

				ep5 {
					reg = <5>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <3>;
					atmel,can-dma;
					atmel,can-isoc;
				};

				ep6 {
					reg = <6>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <3>;
					atmel,can-dma;
					atmel,can-isoc;
				};
			};

			sckc@fffffd50 {
				compatible = "atmel,at91sam9x5-sckc";
				reg = <0xfffffd50 0x4>;

				slow_osc: slow_osc {
					compatible = "atmel,at91sam9x5-clk-slow-osc";
					#clock-cells = <0>;
					atmel,startup-time-usec = <1200000>;
					clocks = <&slow_xtal>;
				};

				slow_rc_osc: slow_rc_osc {
					compatible = "atmel,at91sam9x5-clk-slow-rc-osc";
					#clock-cells = <0>;
					atmel,startup-time-usec = <75>;
					clock-frequency = <32768>;
					clock-accuracy = <50000000>;
				};

				clk32k: slck {
					compatible = "atmel,at91sam9x5-clk-slow";
					#clock-cells = <0>;
					clocks = <&slow_rc_osc &slow_osc>;
				};
			};

			rtc@fffffd20 {
				compatible = "atmel,at91sam9260-rtt";
				reg = <0xfffffd20 0x10>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				clocks = <&clk32k>;
				status = "disabled";
			};

			rtc@fffffdb0 {
				compatible = "atmel,at91rm9200-rtc";
				reg = <0xfffffdb0 0x30>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				clocks = <&clk32k>;
				status = "disabled";
			};

			gpbr: syscon@fffffd60 {
				compatible = "atmel,at91sam9260-gpbr", "syscon";
				reg = <0xfffffd60 0x10>;
				status = "disabled";
			};
		};

		fb0: fb@0x00500000 {
			compatible = "atmel,at91sam9g45-lcdc";
			reg = <0x00500000 0x1000>;
			interrupts = <23 IRQ_TYPE_LEVEL_HIGH 3>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_fb>;
			clocks = <&lcd_clk>, <&lcd_clk>;
			clock-names = "hclk", "lcdc_clk";
			status = "disabled";
		};

		nand0: nand@40000000 {
			compatible = "atmel,at91rm9200-nand";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x40000000 0x10000000
			       0xffffe200 0x200
			      >;
			atmel,nand-addr-offset = <21>;
			atmel,nand-cmd-offset = <22>;
			atmel,nand-has-dma;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_nand>;
			gpios = <&pioC 8 GPIO_ACTIVE_HIGH
				 &pioC 14 GPIO_ACTIVE_HIGH
				 0
				>;
			status = "disabled";
		};

		usb0: ohci@00700000 {
			compatible = "atmel,at91rm9200-ohci", "usb-ohci";
			reg = <0x00700000 0x100000>;
			interrupts = <22 IRQ_TYPE_LEVEL_HIGH 2>;
			clocks = <&uhphs_clk>, <&uhphs_clk>, <&uhpck>;
			clock-names = "ohci_clk", "hclk", "uhpck";
			status = "disabled";
		};

		usb1: ehci@00800000 {
			compatible = "atmel,at91sam9g45-ehci", "usb-ehci";
			reg = <0x00800000 0x100000>;
			interrupts = <22 IRQ_TYPE_LEVEL_HIGH 2>;
			clocks = <&utmi>, <&uhphs_clk>;
			clock-names = "usb_clk", "ehci_clk";
			status = "disabled";
		};
	};

	i2c@0 {
		compatible = "i2c-gpio";
		gpios = <&pioA 20 GPIO_ACTIVE_HIGH /* sda */
			 &pioA 21 GPIO_ACTIVE_HIGH /* scl */
			>;
		i2c-gpio,sda-open-drain;
		i2c-gpio,scl-open-drain;
		i2c-gpio,delay-us = <5>;	/* ~100 kHz */
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};
};
