/*
 * Copyright 2014 - Hans de Goede <hdegoede@redhat.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

/dts-v1/;
#include "sun4i-a10.dtsi"
#include "sunxi-common-regulators.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/sun4i-a10.h>

/ {
	model = "Olimex A10-OLinuXino-LIME";
	compatible = "olimex,a10-olinuxino-lime", "allwinner,sun4i-a10";

	aliases {
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&led_pins_olinuxinolime>;

		green {
			label = "a10-olinuxino-lime:green:usr";
			gpios = <&pio 7 2 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};
	};
};

&ahci {
	target-supply = <&reg_ahci_5v>;
	status = "okay";
};

&cpu0 {
	/*
	 * The A10-Lime is known to be unstable when running at 1008 MHz
	 */
	operating-points = <
		/* kHz    uV */
		912000  1350000
		864000  1300000
		624000  1250000
		>;
	cooling-max-level = <2>;
};

&ehci0 {
	status = "okay";
};

&ehci1 {
	status = "okay";
};

&emac {
	pinctrl-names = "default";
	pinctrl-0 = <&emac_pins_a>;
	phy = <&phy1>;
	status = "okay";
};

&emac_sram {
	status = "okay";
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0_pins_a>;
	status = "okay";

	axp209: pmic@34 {
		compatible = "x-powers,axp209";
		reg = <0x34>;
		interrupts = <0>;

		interrupt-controller;
		#interrupt-cells = <1>;
	};
};

&i2c1 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c1_pins_a>;
	status = "okay";

	eeprom: eeprom@50 {
		compatible = "atmel,24c16";
		reg = <0x50>;
		pagesize = <16>;
	};
};

&mdio {
	status = "okay";

	phy1: ethernet-phy@1 {
		reg = <1>;
	};
};

&mmc0 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin_reference_design>;
	vmmc-supply = <&reg_vcc3v3>;
	bus-width = <4>;
	cd-gpios = <&pio 7 1 GPIO_ACTIVE_HIGH>; /* PH1 */
	cd-inverted;
	status = "okay";
};

&ohci0 {
	status = "okay";
};

&ohci1 {
	status = "okay";
};

&otg_sram {
	status = "okay";
};

&pio {
	ahci_pwr_pin_olinuxinolime: ahci_pwr_pin@1 {
		allwinner,pins = "PC3";
		allwinner,function = "gpio_out";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
	};

	led_pins_olinuxinolime: led_pins@0 {
		allwinner,pins = "PH2";
		allwinner,function = "gpio_out";
		allwinner,drive = <SUN4I_PINCTRL_20_MA>;
		allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
	};

	usb0_id_detect_pin: usb0_id_detect_pin@0 {
		allwinner,pins = "PH4";
		allwinner,function = "gpio_in";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_PULL_UP>;
	};

	usb0_vbus_detect_pin: usb0_vbus_detect_pin@0 {
		allwinner,pins = "PH5";
		allwinner,function = "gpio_in";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_PULL_DOWN>;
	};
};

&reg_ahci_5v {
	pinctrl-0 = <&ahci_pwr_pin_olinuxinolime>;
	gpio = <&pio 2 3 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

&reg_usb0_vbus {
	status = "okay";
};

&reg_usb1_vbus {
	status = "okay";
};

&reg_usb2_vbus {
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pins_a>;
	status = "okay";
};

&usb_otg {
	dr_mode = "otg";
	status = "okay";
};

&usbphy {
	pinctrl-names = "default";
	pinctrl-0 = <&usb0_id_detect_pin>, <&usb0_vbus_detect_pin>;
	usb0_id_det-gpio   = <&pio 7 4 GPIO_ACTIVE_HIGH>; /* PH4 */
	usb0_vbus_det-gpio = <&pio 7 5 GPIO_ACTIVE_HIGH>; /* PH5 */
	usb0_vbus-supply   = <&reg_usb0_vbus>;
	usb1_vbus-supply = <&reg_usb1_vbus>;
	usb2_vbus-supply = <&reg_usb2_vbus>;
	status = "okay";
};
