/*
 * Copyright (C) 2016 Marvell Technology Group Ltd.
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPLv2 or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This library is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This library is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

/*
 * Device Tree file for Marvell Armada CP110 Slave.
 */

#include <dt-bindings/comphy/comphy_data.h>

/ {
	cp110-slave {
		#address-cells = <2>;
		#size-cells = <2>;
		compatible = "simple-bus";
		interrupt-parent = <&gic>;
		ranges;

		config-space {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "simple-bus";
			interrupt-parent = <&gic>;
			ranges = <0x0 0x0 0xf4000000 0x2000000>;

			cps_syscon0: system-controller@440000 {
				compatible = "marvell,cp110-system-controller0",
					     "syscon";
				reg = <0x440000 0x1000>;
				#clock-cells = <2>;
				core-clock-output-names =
					"cps-apll", "cps-ppv2-core", "cps-eip",
					"cps-core", "cps-nand-core";
				gate-clock-output-names =
					"cps-audio", "cps-communit", "cps-nand",
					"cps-ppv2", "cps-sdio", "cps-mg-domain",
					"cps-mg-core", "cps-xor1", "cps-xor0",
					"cps-gop-dp", "none", "cps-pcie_x10",
					"cps-pcie_x11", "cps-pcie_x4", "cps-pcie-xor",
					"cps-sata", "cps-sata-usb", "cps-main",
					"cps-sd-mmc", "none", "none",
					"cps-slow-io", "cps-usb3h0", "cps-usb3h1",
					"cps-usb3dev", "cps-eip150", "cps-eip197";
			};

			cps_pinctl: cps-pinctl@440000 {
				compatible = "marvell,mvebu-pinctrl",
					     "marvell,a80x0-cp1-pinctrl";
				bank-name ="cp1-110";
				reg = <0x440000 0x20>;
				pin-count = <63>;
				max-func = <0xf>;

				cps_ge1_rgmii_pins: cps-ge-rgmii-pins-0 {
					marvell,pins = < 0  1  2  3  4  5  6  7
							 8  9  10 11 >;
					marvell,function = <3>;
				};
				cps_spi1_pins: cps-spi-pins-1 {
					marvell,pins = < 13 14 15 16 >;
					marvell,function = <3>;
				};
			};

			cps_sata0: sata@540000 {
				compatible = "marvell,armada-8k-ahci";
				reg = <0x540000 0x30000>;
				interrupts = <GIC_SPI 287 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&cps_syscon0 1 15>;
				status = "disabled";
			};

			cps_usb3_0: usb3@500000 {
				compatible = "marvell,armada-8k-xhci",
					     "generic-xhci";
				reg = <0x500000 0x4000>;
				dma-coherent;
				interrupts = <GIC_SPI 286 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&cps_syscon0 1 22>;
				status = "disabled";
			};

			cps_usb3_1: usb3@510000 {
				compatible = "marvell,armada-8k-xhci",
					     "generic-xhci";
				reg = <0x510000 0x4000>;
				dma-coherent;
				interrupts = <GIC_SPI 285 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&cps_syscon0 1 23>;
				status = "disabled";
			};

			cps_xor0: xor@6a0000 {
				compatible = "marvell,armada-7k-xor", "marvell,xor-v2";
				reg = <0x6a0000 0x1000>,
				      <0x6b0000 0x1000>;
				dma-coherent;
				msi-parent = <&gic_v2m0>;
				clocks = <&cps_syscon0 1 8>;
			};

			cps_xor1: xor@6c0000 {
				compatible = "marvell,armada-7k-xor", "marvell,xor-v2";
				reg = <0x6c0000 0x1000>,
				      <0x6d0000 0x1000>;
				dma-coherent;
				msi-parent = <&gic_v2m0>;
				clocks = <&cps_syscon0 1 7>;
			};

			cps_spi0: spi@700600 {
				compatible = "marvell,armada-380-spi";
				reg = <0x700600 0x50>;
				#address-cells = <0x1>;
				#size-cells = <0x0>;
				cell-index = <1>;
				clocks = <&cps_syscon0 0 3>;
				status = "disabled";
			};

			cps_spi1: spi@700680 {
				compatible = "marvell,armada-380-spi";
				reg = <0x700680 0x50>;
				#address-cells = <1>;
				#size-cells = <0>;
				cell-index = <2>;
				clocks = <&cps_syscon0 1 21>;
				status = "disabled";
			};

			cps_i2c0: i2c@701000 {
				compatible = "marvell,mv78230-i2c";
				reg = <0x701000 0x20>;
				#address-cells = <1>;
				#size-cells = <0>;
				interrupts = <GIC_SPI 310 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&cps_syscon0 1 21>;
				status = "disabled";
			};

			cps_i2c1: i2c@701100 {
				compatible = "marvell,mv78230-i2c";
				reg = <0x701100 0x20>;
				#address-cells = <1>;
				#size-cells = <0>;
				interrupts = <GIC_SPI 311 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&cps_syscon0 1 21>;
				status = "disabled";
			};

			cps_comphy: comphy@441000 {
				compatible = "marvell,mvebu-comphy", "marvell,comphy-cp110";
				reg = <0x441000 0x8>,
				      <0x120000 0x8>;
				mux-bitcount = <4>;
				max-lanes = <6>;
			};

			cps_utmi0: utmi@580000 {
				compatible = "marvell,mvebu-utmi-2.6.0";
				reg = <0x580000 0x1000>,	/* utmi-unit */
				      <0x440420 0x4>,		/* usb-cfg */
				      <0x440440 0x4>;		/* utmi-cfg */
				utmi-port = <UTMI_PHY_TO_USB_HOST0>;
				status = "disabled";
			};
		};

		cps_pcie0: pcie@f4600000 {
			compatible = "marvell,armada8k-pcie", "snps,dw-pcie";
			reg = <0 0xf4600000 0 0x10000>,
			      <0 0xfaf00000 0 0x80000>;
			reg-names = "ctrl", "config";
			#address-cells = <3>;
			#size-cells = <2>;
			#interrupt-cells = <1>;
			device_type = "pci";
			dma-coherent;
			msi-parent = <&gic_v2m0>;

			bus-range = <0 0xff>;
			ranges =
				/* downstream I/O */
				<0x81000000 0 0xfd000000 0  0xfd000000 0 0x10000
				/* non-prefetchable memory */
				0x82000000 0 0xfa000000 0  0xfa000000 0 0xf00000>;
			interrupt-map-mask = <0 0 0 0>;
			interrupt-map = <0 0 0 0 &gic 0 GIC_SPI 256 IRQ_TYPE_LEVEL_HIGH>;
			interrupts = <GIC_SPI 256 IRQ_TYPE_LEVEL_HIGH>;
			num-lanes = <1>;
			clocks = <&cps_syscon0 1 13>;
			status = "disabled";
		};

		cps_pcie1: pcie@f4620000 {
			compatible = "marvell,armada8k-pcie", "snps,dw-pcie";
			reg = <0 0xf4620000 0 0x10000>,
			      <0 0xfbf00000 0 0x80000>;
			reg-names = "ctrl", "config";
			#address-cells = <3>;
			#size-cells = <2>;
			#interrupt-cells = <1>;
			device_type = "pci";
			dma-coherent;
			msi-parent = <&gic_v2m0>;

			bus-range = <0 0xff>;
			ranges =
				/* downstream I/O */
				<0x81000000 0 0xfd010000 0  0xfd010000 0 0x10000
				/* non-prefetchable memory */
				0x82000000 0 0xfb000000 0  0xfb000000 0 0xf00000>;
			interrupt-map-mask = <0 0 0 0>;
			interrupt-map = <0 0 0 0 &gic 0 GIC_SPI 258 IRQ_TYPE_LEVEL_HIGH>;
			interrupts = <GIC_SPI 258 IRQ_TYPE_LEVEL_HIGH>;

			num-lanes = <1>;
			clocks = <&cps_syscon0 1 11>;
			status = "disabled";
		};

		cps_pcie2: pcie@f4640000 {
			compatible = "marvell,armada8k-pcie", "snps,dw-pcie";
			reg = <0 0xf4640000 0 0x10000>,
			      <0 0xfcf00000 0 0x80000>;
			reg-names = "ctrl", "config";
			#address-cells = <3>;
			#size-cells = <2>;
			#interrupt-cells = <1>;
			device_type = "pci";
			dma-coherent;
			msi-parent = <&gic_v2m0>;

			bus-range = <0 0xff>;
			ranges =
				/* downstream I/O */
				<0x81000000 0 0xfd020000 0  0xfd020000 0 0x10000
				/* non-prefetchable memory */
				0x82000000 0 0xfc000000 0  0xfc000000 0 0xf00000>;
			interrupt-map-mask = <0 0 0 0>;
			interrupt-map = <0 0 0 0 &gic 0 GIC_SPI 257 IRQ_TYPE_LEVEL_HIGH>;
			interrupts = <GIC_SPI 257 IRQ_TYPE_LEVEL_HIGH>;

			num-lanes = <1>;
			clocks = <&cps_syscon0 1 12>;
			status = "disabled";
		};
	};
};
