/*
 * Copyright (C) 2016 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
#include "dra72-evm-common.dtsi"
#include <dt-bindings/net/ti-dp83867.h>

/ {
	model = "TI DRA722 Rev C EVM";

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x80000000 0x0 0x80000000>; /* 2GB */
	};
};

&i2c1 {
	tps65917: tps65917@58 {
		reg = <0x58>;

		interrupts = <GIC_SPI 2 IRQ_TYPE_NONE>;  /* IRQ_SYS_1N */
	};
};

#include "dra72-evm-tps65917.dtsi"

&ldo2_reg {
	/* LDO2_OUT --> VDDA_1V8_PHY2 */
	regulator-always-on;
	regulator-boot-on;
};

&hdmi {
	vdda-supply = <&ldo2_reg>;
};

&pcf_gpio_21 {
	interrupt-parent = <&gpio3>;
	interrupts = <30 IRQ_TYPE_EDGE_FALLING>;
};

&mac {
	mode-gpios = <&pcf_gpio_21 4 GPIO_ACTIVE_LOW>,
		     <&pcf_hdmi 9 GPIO_ACTIVE_LOW>,	/* P11 */
		     <&pcf_hdmi 10 GPIO_ACTIVE_LOW>;	/* P12 */
	dual_emac;
};

&cpsw_emac0 {
	phy-handle = <&dp83867_0>;
	phy-mode = "rgmii-id";
	dual_emac_res_vlan = <1>;
};

&cpsw_emac1 {
	phy-handle = <&dp83867_1>;
	phy-mode = "rgmii-id";
	dual_emac_res_vlan = <2>;
};

&davinci_mdio {
	dp83867_0: ethernet-phy@2 {
		reg = <2>;
		ti,rx-internal-delay = <DP83867_RGMIIDCTL_2_25_NS>;
		ti,tx-internal-delay = <DP83867_RGMIIDCTL_250_PS>;
		ti,fifo-depth = <DP83867_PHYCR_FIFO_DEPTH_8_B_NIB>;
		ti,min-output-imepdance;
	};

	dp83867_1: ethernet-phy@3 {
		reg = <3>;
		ti,rx-internal-delay = <DP83867_RGMIIDCTL_2_25_NS>;
		ti,tx-internal-delay = <DP83867_RGMIIDCTL_250_PS>;
		ti,fifo-depth = <DP83867_PHYCR_FIFO_DEPTH_8_B_NIB>;
		ti,min-output-imepdance;
	};
};
