/*
 * Copyright (C) 2016 Marvell Technology Group Ltd.
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPLv2 or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This library is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This library is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

/*
 * Device Tree file for Marvell Armada 7040 Development board platform
 */

#include "armada-7040.dtsi"

/ {
	model = "Marvell Armada 7040 DB board";
	compatible = "marvell,armada7040-db", "marvell,armada7040",
		     "marvell,armada-ap806-quad", "marvell,armada-ap806";

	chosen {
		stdout-path = "serial0:115200n8";
	};

	aliases {
		i2c0 = &cpm_i2c0;
		spi0 = &cpm_spi1;
	};

	memory@00000000 {
		device_type = "memory";
		reg = <0x0 0x0 0x0 0x80000000>;
	};
};

&ap_pinctl {
	   /* MPP Bus:
	    * SDIO  [0-5]
	    * UART0 [11,19]
	    */
		  /* 0 1 2 3 4 5 6 7 8 9 */
	pin-func = < 1 1 1 1 1 1 0 0 0 0
		     0 3 0 0 0 0 0 0 0 3 >;
};

&uart0 {
	status = "okay";
};


&cpm_pcie2 {
	status = "okay";
};

&cpm_i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&cpm_i2c0_pins>;
	status = "okay";
	clock-frequency = <100000>;
};

&cpm_pinctl {
		/* MPP Bus:
		 * TDM	 [0-11]
		 * SPI   [13-16]
		 * SATA1 [28]
		 * UART0 [29-30]
		 * SMI	 [32,34]
		 * XSMI  [35-36]
		 * I2C	 [37-38]
		 * RGMII1[44-55]
		 * SD	 [56-62]
		 */
		/*   0   1   2   3   4   5   6   7   8   9 */
	pin-func = < 4   4   4   4   4   4   4   4   4   4
		     4   4   0   3   3   3   3   0   0   0
		     0   0   0   0   0   0   0   0   9   0xA
		     0xA 0   7   0   7   7   7   2   2   0
		     0   0   0   0   1   1   1   1   1   1
		     1   1   1   1   1   1   0xE 0xE 0xE 0xE
		     0xE 0xE 0xE >;
};

&cpm_spi1 {
	pinctrl-names = "default";
	pinctrl-0 = <&cpm_spi0_pins>;
	status = "okay";

	spi-flash@0 {
		#address-cells = <0x1>;
		#size-cells = <0x1>;
		compatible = "jedec,spi-nor";
		reg = <0x0>;
		spi-max-frequency = <20000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "U-Boot";
				reg = <0x0 0x200000>;
			};

			partition@400000 {
				label = "Filesystem";
				reg = <0x200000 0xe00000>;
			};
		};
	};
};

&cpm_sata0 {
	status = "okay";
};

&cpm_usb3_0 {
	status = "okay";
};

&cpm_usb3_1 {
	status = "okay";
};

&cpm_comphy {
	phy0 {
		phy-type = <PHY_TYPE_SGMII2>;
		phy-speed = <PHY_SPEED_3_125G>;
	};

	phy1 {
		phy-type = <PHY_TYPE_USB3_HOST0>;
		phy-speed = <PHY_SPEED_5G>;
	};

	phy2 {
		phy-type = <PHY_TYPE_SGMII0>;
		phy-speed = <PHY_SPEED_1_25G>;
	};

	phy3 {
		phy-type = <PHY_TYPE_SATA1>;
		phy-speed = <PHY_SPEED_5G>;
	};

	phy4 {
		phy-type = <PHY_TYPE_USB3_HOST1>;
		phy-speed = <PHY_SPEED_5G>;
	};

	phy5 {
		phy-type = <PHY_TYPE_PEX2>;
		phy-speed = <PHY_SPEED_5G>;
	};
};

&cpm_utmi0 {
	status = "okay";
};

&cpm_utmi1 {
	status = "okay";
};
