/*
 * Copyright (C) 2014 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 * Based on "omap4.dtsi"
 */

#include "dra7.dtsi"

/ {
	compatible = "ti,dra742", "ti,dra74", "ti,dra7";

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <0>;

			operating-points = <
				/* kHz    uV */
				1000000	1060000
				1176000	1160000
				>;

			clocks = <&dpll_mpu_ck>;
			clock-names = "cpu";

			clock-latency = <300000>; /* From omap-cpufreq driver */

			/* cooling options */
			cooling-min-level = <0>;
			cooling-max-level = <2>;
			#cooling-cells = <2>; /* min followed by max */
		};
		cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <1>;
		};
	};

	pmu {
		compatible = "arm,cortex-a15-pmu";
		interrupt-parent = <&wakeupgen>;
		interrupts = <GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 132 IRQ_TYPE_LEVEL_HIGH>;
	};

	ocp {
		omap_dwc3_4: omap_dwc3_4@48940000 {
			compatible = "ti,dwc3";
			ti,hwmods = "usb_otg_ss4";
			reg = <0x48940000 0x10000>;
			interrupts = <GIC_SPI 346 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <1>;
			utmi-mode = <2>;
			ranges;
			status = "disabled";
			usb4: usb@48950000 {
				compatible = "snps,dwc3";
				reg = <0x48950000 0x17000>;
				interrupts = <GIC_SPI 345 IRQ_TYPE_LEVEL_HIGH>;
				tx-fifo-resize;
				maximum-speed = "high-speed";
				dr_mode = "otg";
			};
		};
	};
};

&dss {
	reg = <0x58000000 0x80>,
	      <0x58004054 0x4>,
	      <0x58004300 0x20>,
	      <0x58005054 0x4>,
	      <0x58005300 0x20>;
	reg-names = "dss", "pll1_clkctrl", "pll1",
		    "pll2_clkctrl", "pll2";

	clocks = <&dss_dss_clk>,
		 <&dss_video1_clk>,
		 <&dss_video2_clk>;
	clock-names = "fck", "video1_clk", "video2_clk";
};
