#include "bcm283x.dtsi"

/ {
	compatible = "brcm,bcm2836";

	soc {
		ranges = <0x7e000000 0x3f000000 0x1000000>,
			 <0x40000000 0x40000000 0x00001000>;
		dma-ranges = <0xc0000000 0x00000000 0x3f000000>;

		local_intc: local_intc {
			compatible = "brcm,bcm2836-l1-intc";
			reg = <0x40000000 0x100>;
			interrupt-controller;
			#interrupt-cells = <1>;
			interrupt-parent = <&local_intc>;
		};
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupt-parent = <&local_intc>;
		interrupts = <0>, // PHYS_SECURE_PPI
			     <1>, // PHYS_NONSECURE_PPI
			     <3>, // VIRT_PPI
			     <2>; // HYP_PPI
		always-on;
	};

	cpus: cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0>;
			enable-method = "spin-table";
			cpu-release-addr = <0x0 0x000000d8>;
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <1>;
			enable-method = "spin-table";
			cpu-release-addr = <0x0 0x000000e0>;
		};

		cpu2: cpu@2 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <2>;
			enable-method = "spin-table";
			cpu-release-addr = <0x0 0x000000e8>;
		};

		cpu3: cpu@3 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <3>;
			enable-method = "spin-table";
			cpu-release-addr = <0x0 0x000000f0>;
		};
	};
};

/* Make the BCM2835-style global interrupt controller be a child of the
 * CPU-local interrupt controller.
 */
&intc {
	compatible = "brcm,bcm2836-armctrl-ic";
	reg = <0x7e00b200 0x200>;
	interrupt-parent = <&local_intc>;
	interrupts = <8>;
};
