/*
 * Copyright 2015 Hans de Goede <hdegoede@redhat.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

/dts-v1/;
#include "sun7i-a20.dtsi"
#include "sunxi-common-regulators.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>

/ {
	model = "LeMaker Banana Pro";
	compatible = "lemaker,bananapro", "allwinner,sun7i-a20";

	aliases {
		serial0 = &uart0;
		serial1 = &uart4;
		serial2 = &uart7;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&led_pins_bananapro>;

		blue {
			label = "bananapro:blue:usr";
			gpios = <&pio 6 2 GPIO_ACTIVE_HIGH>;
		};

		green {
			label = "bananapro:green:usr";
			gpios = <&pio 7 24 GPIO_ACTIVE_HIGH>;
		};
	};

	reg_gmac_3v3: gmac-3v3 {
		compatible = "regulator-fixed";
		pinctrl-names = "default";
		pinctrl-0 = <&gmac_power_pin_bananapro>;
		regulator-name = "gmac-3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		startup-delay-us = <100000>;
		enable-active-high;
		gpio = <&pio 7 23 GPIO_ACTIVE_HIGH>;
	};

	reg_vmmc3: vmmc3 {
		compatible = "regulator-fixed";
		pinctrl-names = "default";
		pinctrl-0 = <&vmmc3_pin_bananapro>;
		regulator-name = "vmmc3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		enable-active-high;
		gpio = <&pio 7 22 GPIO_ACTIVE_HIGH>;
	};
};

&ahci {
	status = "okay";
};

&ehci0 {
	status = "okay";
};

&ehci1 {
	status = "okay";
};

&gmac {
	pinctrl-names = "default";
	pinctrl-0 = <&gmac_pins_rgmii_a>;
	phy = <&phy1>;
	phy-mode = "rgmii";
	phy-supply = <&reg_gmac_3v3>;
	status = "okay";

	phy1: ethernet-phy@1 {
		reg = <1>;
	};
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0_pins_a>;
	status = "okay";

	axp209: pmic@34 {
		compatible = "x-powers,axp209";
		reg = <0x34>;
		interrupt-parent = <&nmi_intc>;
		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;

		interrupt-controller;
		#interrupt-cells = <1>;
	};
};

&i2c2 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c2_pins_a>;
	status = "okay";
};

&ir0 {
	pinctrl-names = "default";
	pinctrl-0 = <&ir0_rx_pins_a>;
	status = "okay";
};

&mmc0 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin_bananapro>;
	vmmc-supply = <&reg_vcc3v3>;
	bus-width = <4>;
	cd-gpios = <&pio 7 10 GPIO_ACTIVE_HIGH>; /* PH10 */
	cd-inverted;
	status = "okay";
};

&mmc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc3_pins_a>;
	vmmc-supply = <&reg_vmmc3>;
	bus-width = <4>;
	non-removable;
	status = "okay";
};

&ohci0 {
	status = "okay";
};

&ohci1 {
	status = "okay";
};

&pio {
	gmac_power_pin_bananapro: gmac_power_pin@0 {
		allwinner,pins = "PH23";
		allwinner,function = "gpio_out";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
	};

	led_pins_bananapro: led_pins@0 {
		allwinner,pins = "PH24", "PG2";
		allwinner,function = "gpio_out";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
	};

	mmc0_cd_pin_bananapro: mmc0_cd_pin@0 {
		allwinner,pins = "PH10";
		allwinner,function = "gpio_in";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_PULL_UP>;
	};

	usb1_vbus_pin_bananapro: usb1_vbus_pin@0 {
		allwinner,pins = "PH0";
		allwinner,function = "gpio_out";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
	};

	usb2_vbus_pin_bananapro: usb2_vbus_pin@0 {
		allwinner,pins = "PH1";
		allwinner,function = "gpio_out";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
	};

	vmmc3_pin_bananapro: vmmc3_pin@0 {
		allwinner,pins = "PH22";
		allwinner,function = "gpio_out";
		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
		allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
	};
};

&reg_usb1_vbus {
	pinctrl-0 = <&usb1_vbus_pin_bananapro>;
	gpio = <&pio 7 0 GPIO_ACTIVE_HIGH>; /* PH0 */
	status = "okay";
};

&reg_usb2_vbus {
	pinctrl-0 = <&usb2_vbus_pin_bananapro>;
	gpio = <&pio 7 1 GPIO_ACTIVE_HIGH>; /* PH1 */
	status = "okay";
};

&spi0 {
	pinctrl-names = "default";
	pinctrl-0 = <&spi0_pins_a>,
		    <&spi0_cs0_pins_a>,
		    <&spi0_cs1_pins_a>;
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pins_a>;
	status = "okay";
};

&uart4 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart4_pins_b>;
	status = "okay";
};

&uart7 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart7_pins_a>;
	status = "okay";
};

&usbphy {
	usb1_vbus-supply = <&reg_usb1_vbus>;
	usb2_vbus-supply = <&reg_usb2_vbus>;
	status = "okay";
};
