/*
 * Copyright (C) 2012 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
/dts-v1/;

#include "am33xx.dtsi"
#include "am335x-bone-common.dtsi"

/ {
	model = "TI AM335x BeagleBone Green";
	compatible = "ti,am335x-bone-green", "ti,am335x-bone-black", "ti,am335x-bone", "ti,am33xx";
	chosen {
		stdout-path = &uart0;
		tick-timer = &timer2;
	};
};

&ldo3_reg {
	regulator-min-microvolt = <1800000>;
	regulator-max-microvolt = <1800000>;
	regulator-always-on;
};

&mmc1 {
	vmmc-supply = <&vmmcsd_fixed>;
};

&mmc2 {
	vmmc-supply = <&vmmcsd_fixed>;
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_pins>;
	bus-width = <8>;
	status = "okay";
};

&am33xx_pinmux {
	uart2_pins: uart2_pins {
		pinctrl-single,pins = <
			AM33XX_IOPAD(0x950, PIN_INPUT | MUX_MODE1)	/* spi0_sclk.uart2_rxd */
			AM33XX_IOPAD(0x954, PIN_OUTPUT | MUX_MODE1)	/* spi0_d0.uart2_txd */
		>;
	};
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart2_pins>;
	status = "okay";
};

&rtc {
	system-power-controller;
};
