/*
 * Device Tree Include file for Freescale Layerscape-1043A family SoC.
 *
 * Copyright (C) 2014-2015, Freescale Semiconductor
 *
 * Mingkai Hu <Mingkai.hu@freescale.com>
 *
 * This file is licensed under the terms of the GNU General Public
 * License version 2.  This program is licensed "as is" without any
 * warranty of any kind, whether express or implied.
 */

/include/ "skeleton64.dtsi"

/ {
	compatible = "fsl,ls1043a";
	interrupt-parent = <&gic>;

	sysclk: sysclk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <100000000>;
		clock-output-names = "sysclk";
	};

	gic: interrupt-controller@1400000 {
		compatible = "arm,gic-400";
		#interrupt-cells = <3>;
		interrupt-controller;
		reg = <0x0 0x1401000 0 0x1000>, /* GICD */
		      <0x0 0x1402000 0 0x2000>, /* GICC */
		      <0x0 0x1404000 0 0x2000>, /* GICH */
		      <0x0 0x1406000 0 0x2000>; /* GICV */
		interrupts = <1 9 0xf08>;
	};

	soc {
		compatible = "simple-bus";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		clockgen: clocking@1ee1000 {
			compatible = "fsl,ls1043a-clockgen";
			reg = <0x0 0x1ee1000 0x0 0x1000>;
			#clock-cells = <2>;
			clocks = <&sysclk>;
		};

		dspi0: dspi@2100000 {
			compatible = "fsl,vf610-dspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2100000 0x0 0x10000>;
			interrupts = <0 64 0x4>;
			clock-names = "dspi";
			clocks = <&clockgen 4 0>;
			num-cs = <6>;
			big-endian;
			status = "disabled";
		};

		dspi1: dspi@2110000 {
			compatible = "fsl,vf610-dspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2110000 0x0 0x10000>;
			interrupts = <0 65 0x4>;
			clock-names = "dspi";
			clocks = <&clockgen 4 0>;
			num-cs = <6>;
			big-endian;
			status = "disabled";
		};

		ifc: ifc@1530000 {
			compatible = "fsl,ifc", "simple-bus";
			reg = <0x0 0x1530000 0x0 0x10000>;
			interrupts = <0 43 0x4>;
		};

		i2c0: i2c@2180000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2180000 0x0 0x10000>;
			interrupts = <0 56 0x4>;
			clock-names = "i2c";
			clocks = <&clockgen 4 0>;
			status = "disabled";
		};

		i2c1: i2c@2190000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2190000 0x0 0x10000>;
			interrupts = <0 57 0x4>;
			clock-names = "i2c";
			clocks = <&clockgen 4 0>;
			status = "disabled";
		};

		i2c2: i2c@21a0000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x21a0000 0x0 0x10000>;
			interrupts = <0 58 0x4>;
			clock-names = "i2c";
			clocks = <&clockgen 4 0>;
			status = "disabled";
		};

		i2c3: i2c@21b0000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x21b0000 0x0 0x10000>;
			interrupts = <0 59 0x4>;
			clock-names = "i2c";
			clocks = <&clockgen 4 0>;
			status = "disabled";
		};

		duart0: serial@21c0500 {
			compatible = "fsl,ns16550", "ns16550a";
			reg = <0x00 0x21c0500 0x0 0x100>;
			interrupts = <0 54 0x4>;
			clocks = <&clockgen 4 0>;
		};

		duart1: serial@21c0600 {
			compatible = "fsl,ns16550", "ns16550a";
			reg = <0x00 0x21c0600 0x0 0x100>;
			interrupts = <0 54 0x4>;
			clocks = <&clockgen 4 0>;
		};

		duart2: serial@21d0500 {
			compatible = "fsl,ns16550", "ns16550a";
			reg = <0x0 0x21d0500 0x0 0x100>;
			interrupts = <0 55 0x4>;
			clocks = <&clockgen 4 0>;
		};

		duart3: serial@21d0600 {
			compatible = "fsl,ns16550", "ns16550a";
			reg = <0x0 0x21d0600 0x0 0x100>;
			interrupts = <0 55 0x4>;
			clocks = <&clockgen 4 0>;
		};

		lpuart0: serial@2950000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x2950000 0x0 0x1000>;
			interrupts = <0 48 0x4>;
			clocks = <&sysclk>;
			clock-names = "ipg";
			status = "disabled";
		};

		lpuart1: serial@2960000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x2960000 0x0 0x1000>;
			interrupts = <0 49 0x4>;
			clocks = <&sysclk>;
			clock-names = "ipg";
			status = "disabled";
		};

		lpuart2: serial@2970000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x2970000 0x0 0x1000>;
			interrupts = <0 50 0x4>;
			clock-names = "ipg";
			clocks = <&sysclk>;
			status = "disabled";
		};

		lpuart3: serial@2980000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x2980000 0x0 0x1000>;
			interrupts = <0 51 0x4>;
			clocks = <&sysclk>;
			clock-names = "ipg";
			status = "disabled";
		};

		lpuart4: serial@2990000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x2990000 0x0 0x1000>;
			interrupts = <0 52 0x4>;
			clocks = <&sysclk>;
			clock-names = "ipg";
			status = "disabled";
		};

		lpuart5: serial@29a0000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x29a0000 0x0 0x1000>;
			interrupts = <0 53 0x4>;
			clocks = <&sysclk>;
			clock-names = "ipg";
			status = "disabled";
		};
		qspi: quadspi@1550000 {
			compatible = "fsl,vf610-qspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x1550000 0x0 0x10000>,
				<0x0 0x40000000 0x0 0x4000000>;
			reg-names = "QuadSPI", "QuadSPI-memory";
			num-cs = <2>;
			big-endian;
			status = "disabled";
		};

		usb0: usb3@2f00000 {
			compatible = "fsl,layerscape-dwc3";
			reg = <0x0 0x2f00000 0x0 0x10000>;
			interrupts = <0 60 0x4>;
			dr_mode = "host";
		};

		usb1: usb3@3000000 {
			compatible = "fsl,layerscape-dwc3";
			reg = <0x0 0x3000000 0x0 0x10000>;
			interrupts = <0 61 0x4>;
			dr_mode = "host";
		};

		usb2: usb3@3100000 {
			compatible = "fsl,layerscape-dwc3";
			reg = <0x0 0x3100000 0x0 0x10000>;
			interrupts = <0 63 0x4>;
			dr_mode = "host";
		};
	};
};
