/*
 * dts file for Xilinx ZynqMP zc1751-xm018-dc4
 *
 * (C) Copyright 2015 - 2016, Xilinx, Inc.
 *
 * Michal Simek <michal.simek@xilinx.com>
 *
 * This program is free software; you can redistribute it and/or
 * modify it under the terms of the GNU General Public License as
 * published by the Free Software Foundation; either version 2 of
 * the License, or (at your option) any later version.
 */

/dts-v1/;

#include "zynqmp.dtsi"
#include "zynqmp-clk.dtsi"

/ {
	model = "ZynqMP zc1751-xm018-dc4";
	compatible = "xlnx,zynqmp-zc1751", "xlnx,zynqmp";

	aliases {
		can0 = &can0;
		can1 = &can1;
		ethernet0 = &gem0;
		ethernet1 = &gem1;
		ethernet2 = &gem2;
		ethernet3 = &gem3;
		gpio0 = &gpio;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		rtc0 = &rtc;
		serial0 = &uart0;
		serial1 = &uart1;
		spi0 = &qspi;
	};

	chosen {
		bootargs = "earlycon";
		stdout-path = "serial0:115200n8";
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x0 0x0 0x80000000>, <0x8 0x00000000 0x0 0x80000000>;
	};
};

&can0 {
	status = "okay";
};

&can1 {
	status = "okay";
};

/* fpd_dma clk 667MHz, lpd_dma 500MHz */
&fpd_dma_chan1 {
	status = "okay";
	xlnx,include-sg; /* for testing purpose */
	xlnx,overfetch; /* for testing purpose */
	xlnx,ratectrl = <0>; /* for testing purpose */
	xlnx,src-issue = <31>;
};

&fpd_dma_chan2 {
	status = "okay";
	xlnx,ratectrl = <100>; /* for testing purpose */
	xlnx,src-issue = <4>; /* for testing purpose */
};

&fpd_dma_chan3 {
	status = "okay";
};

&fpd_dma_chan4 {
	status = "okay";
	xlnx,include-sg; /* for testing purpose */
};

&fpd_dma_chan5 {
	status = "okay";
};

&fpd_dma_chan6 {
	status = "okay";
	xlnx,include-sg; /* for testing purpose */
};

&fpd_dma_chan7 {
	status = "okay";
};

&fpd_dma_chan8 {
	status = "okay";
	xlnx,include-sg; /* for testing purpose */
};

&lpd_dma_chan1 {
	status = "okay";
};

&lpd_dma_chan2 {
	status = "okay";
};

&lpd_dma_chan3 {
	status = "okay";
};

&lpd_dma_chan4 {
	status = "okay";
};

&lpd_dma_chan5 {
	status = "okay";
};

&lpd_dma_chan6 {
	status = "okay";
};

&lpd_dma_chan7 {
	status = "okay";
};

&lpd_dma_chan8 {
	status = "okay";
};

&xlnx_dp {
	status = "okay";
};

&xlnx_dpdma {
	status = "okay";
};

&gem0 {
	status = "okay";
	local-mac-address = [00 0a 35 00 02 90];
	phy-mode = "rgmii-id";
	phy-handle = <&ethernet_phy0>;
	ethernet_phy0: ethernet-phy@0 { /* Marvell 88e1512 */
		reg = <0>;
	};
	ethernet_phy7: ethernet-phy@7 { /* Vitesse VSC8211 */
		reg = <7>;
	};
	ethernet_phy3: ethernet-phy@3 { /* Realtek RTL8211DN */
		reg = <3>;
	};
	ethernet_phy8: ethernet-phy@8 { /* Vitesse VSC8211 */
		reg = <8>;
	};
};

&gem1 {
	status = "okay";
	local-mac-address = [00 0a 35 00 02 91];
	phy-mode = "rgmii-id";
	phy-handle = <&ethernet_phy7>;
};

&gem2 {
	status = "okay";
	local-mac-address = [00 0a 35 00 02 92];
	phy-mode = "rgmii-id";
	phy-handle = <&ethernet_phy3>;
};

&gem3 {
	status = "okay";
	local-mac-address = [00 0a 35 00 02 93];
	phy-mode = "rgmii-id";
	phy-handle = <&ethernet_phy8>;
};

&gpio {
	status = "okay";
};

&gpu {
	status = "okay";
};

&i2c0 {
	clock-frequency = <400000>;
	status = "okay";
};

&i2c1 {
	clock-frequency = <400000>;
	status = "okay";
};

&rtc {
	status = "okay";
};

&uart0 {
	status = "okay";
};

&uart1 {
	status = "okay";
};

&watchdog0 {
	status = "okay";
};
