/dts-v1/;
#include "bcm2835.dtsi"
#include "bcm2835-rpi.dtsi"
#include "bcm283x-rpi-smsc9512.dtsi"

/ {
	compatible = "raspberrypi,model-b", "brcm,bcm2835";
	model = "Raspberry Pi Model B";

	leds {
		act {
			gpios = <&gpio 16 1>;
		};
	};
};

&gpio {
	pinctrl-0 = <&gpioout &alt0 &alt3>;
};

&hdmi {
	hpd-gpios = <&gpio 46 GPIO_ACTIVE_HIGH>;
};
