/*
 * dts file for Xilinx ZynqMP
 *
 * (C) Copyright 2014 - 2015, Xilinx, Inc.
 *
 * Michal Simek <michal.simek@xilinx.com>
 *
 * SPDX-License-Identifier:	GPL-2.0+
 */

/ {
	compatible = "xlnx,zynqmp";
	#address-cells = <2>;
	#size-cells = <2>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			compatible = "arm,cortex-a53", "arm,armv8";
			device_type = "cpu";
			enable-method = "psci";
			reg = <0x0>;
		};

		cpu@1 {
			compatible = "arm,cortex-a53", "arm,armv8";
			device_type = "cpu";
			enable-method = "psci";
			reg = <0x1>;
		};

		cpu@2 {
			compatible = "arm,cortex-a53", "arm,armv8";
			device_type = "cpu";
			enable-method = "psci";
			reg = <0x2>;
		};

		cpu@3 {
			compatible = "arm,cortex-a53", "arm,armv8";
			device_type = "cpu";
			enable-method = "psci";
			reg = <0x3>;
		};
	};

	dcc: dcc {
		compatible = "arm,dcc";
		status = "disabled";
		u-boot,dm-pre-reloc;
	};

	power-domains {
		compatible = "xlnx,zynqmp-genpd";

		pd_usb0: pd-usb0 {
			#power-domain-cells = <0x0>;
			pd-id = <0x16>;
		};

		pd_usb1: pd-usb1 {
			#power-domain-cells = <0x0>;
			pd-id = <0x17>;
		};

		pd_sata: pd-sata {
			#power-domain-cells = <0x0>;
			pd-id = <0x1c>;
		};

		pd_spi0: pd-spi0 {
			#power-domain-cells = <0x0>;
			pd-id = <0x23>;
		};

		pd_spi1: pd-spi1 {
			#power-domain-cells = <0x0>;
			pd-id = <0x24>;
		};

		pd_uart0: pd-uart0 {
			#power-domain-cells = <0x0>;
			pd-id = <0x21>;
		};

		pd_uart1: pd-uart1 {
			#power-domain-cells = <0x0>;
			pd-id = <0x22>;
		};

		pd_eth0: pd-eth0 {
			#power-domain-cells = <0x0>;
			pd-id = <0x1d>;
		};

		pd_eth1: pd-eth1 {
			#power-domain-cells = <0x0>;
			pd-id = <0x1e>;
		};

		pd_eth2: pd-eth2 {
			#power-domain-cells = <0x0>;
			pd-id = <0x1f>;
		};

		pd_eth3: pd-eth3 {
			#power-domain-cells = <0x0>;
			pd-id = <0x20>;
		};

		pd_i2c0: pd-i2c0 {
			#power-domain-cells = <0x0>;
			pd-id = <0x25>;
		};

		pd_i2c1: pd-i2c1 {
			#power-domain-cells = <0x0>;
			pd-id = <0x26>;
		};

		pd_dp: pd-dp {
			/* fixme: what to attach to */
			#power-domain-cells = <0x0>;
			pd-id = <0x29>;
		};

		pd_gdma: pd-gdma {
			#power-domain-cells = <0x0>;
			pd-id = <0x2a>;
		};

		pd_adma: pd-adma {
			#power-domain-cells = <0x0>;
			pd-id = <0x2b>;
		};

		pd_ttc0: pd-ttc0 {
			#power-domain-cells = <0x0>;
			pd-id = <0x18>;
		};

		pd_ttc1: pd-ttc1 {
			#power-domain-cells = <0x0>;
			pd-id = <0x19>;
		};

		pd_ttc2: pd-ttc2 {
			#power-domain-cells = <0x0>;
			pd-id = <0x1a>;
		};

		pd_ttc3: pd-ttc3 {
			#power-domain-cells = <0x0>;
			pd-id = <0x1b>;
		};

		pd_sd0: pd-sd0 {
			#power-domain-cells = <0x0>;
			pd-id = <0x27>;
		};

		pd_sd1: pd-sd1 {
			#power-domain-cells = <0x0>;
			pd-id = <0x28>;
		};

		pd_nand: pd-nand {
			#power-domain-cells = <0x0>;
			pd-id = <0x2c>;
		};

		pd_qspi: pd-qspi {
			#power-domain-cells = <0x0>;
			pd-id = <0x2d>;
		};

		pd_gpio: pd-gpio {
			#power-domain-cells = <0x0>;
			pd-id = <0x2e>;
		};

		pd_can0: pd-can0 {
			#power-domain-cells = <0x0>;
			pd-id = <0x2f>;
		};

		pd_can1: pd-can1 {
			#power-domain-cells = <0x0>;
			pd-id = <0x30>;
		};

		pd_pcie: pd-pcie {
			#power-domain-cells = <0x0>;
			pd-id = <0x3b>;
		};

		pd_gpu: pd-gpu {
			#power-domain-cells = <0x0>;
			pd-id = <0x3a 0x14 0x15>;
		};
	};

	pmu {
		compatible = "arm,armv8-pmuv3";
		interrupt-parent = <&gic>;
		interrupts = <0 143 4>,
			     <0 144 4>,
			     <0 145 4>,
			     <0 146 4>;
	};

	psci {
		compatible = "arm,psci-0.2";
		method = "smc";
	};

	firmware {
		compatible = "xlnx,zynqmp-pm";
		method = "smc";
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupt-parent = <&gic>;
		interrupts = <1 13 0xf01>,
			     <1 14 0xf01>,
			     <1 11 0xf01>,
			     <1 10 0xf01>;
	};

	edac {
		compatible = "arm,cortex-a53-edac";
	};

	pcap {
		compatible = "xlnx,zynqmp-pcap-fpga";
	};

	amba_apu: amba_apu@0 {
		compatible = "simple-bus";
		#address-cells = <2>;
		#size-cells = <1>;
		ranges = <0 0 0 0 0xffffffff>;

		gic: interrupt-controller@f9010000 {
			compatible = "arm,gic-400", "arm,cortex-a15-gic";
			#interrupt-cells = <3>;
			reg = <0x0 0xf9010000 0x10000>,
			      <0x0 0xf9020000 0x20000>,
			      <0x0 0xf9040000 0x20000>,
			      <0x0 0xf9060000 0x20000>;
			interrupt-controller;
			interrupt-parent = <&gic>;
			interrupts = <1 9 0xf04>;
		};
	};

	amba: amba {
		compatible = "simple-bus";
		u-boot,dm-pre-reloc;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		can0: can@ff060000 {
			compatible = "xlnx,zynq-can-1.0";
			status = "disabled";
			clock-names = "can_clk", "pclk";
			reg = <0x0 0xff060000 0x0 0x1000>;
			interrupts = <0 23 4>;
			interrupt-parent = <&gic>;
			tx-fifo-depth = <0x40>;
			rx-fifo-depth = <0x40>;
			power-domains = <&pd_can0>;
		};

		can1: can@ff070000 {
			compatible = "xlnx,zynq-can-1.0";
			status = "disabled";
			clock-names = "can_clk", "pclk";
			reg = <0x0 0xff070000 0x0 0x1000>;
			interrupts = <0 24 4>;
			interrupt-parent = <&gic>;
			tx-fifo-depth = <0x40>;
			rx-fifo-depth = <0x40>;
			power-domains = <&pd_can1>;
		};

		cci: cci@fd6e0000 {
			compatible = "arm,cci-400";
			reg = <0x0 0xfd6e0000 0x0 0x9000>;
			ranges = <0x0 0x0 0xfd6e0000 0x10000>;
			#address-cells = <1>;
			#size-cells = <1>;

			pmu@9000 {
				compatible = "arm,cci-400-pmu,r1";
				reg = <0x9000 0x5000>;
				interrupt-parent = <&gic>;
				interrupts = <0 123 4>,
					     <0 123 4>,
					     <0 123 4>,
					     <0 123 4>,
					     <0 123 4>;
			};
		};

		/* GDMA */
		fpd_dma_chan1: dma@fd500000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			reg = <0x0 0xfd500000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 124 4>;
			clock-names = "clk_main", "clk_apb";
			xlnx,bus-width = <128>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x14e8>;
			power-domains = <&pd_gdma>;
		};

		fpd_dma_chan2: dma@fd510000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			reg = <0x0 0xfd510000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 125 4>;
			clock-names = "clk_main", "clk_apb";
			xlnx,bus-width = <128>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x14e9>;
			power-domains = <&pd_gdma>;
		};

		fpd_dma_chan3: dma@fd520000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			reg = <0x0 0xfd520000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 126 4>;
			clock-names = "clk_main", "clk_apb";
			xlnx,bus-width = <128>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x14ea>;
			power-domains = <&pd_gdma>;
		};

		fpd_dma_chan4: dma@fd530000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			reg = <0x0 0xfd530000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 127 4>;
			clock-names = "clk_main", "clk_apb";
			xlnx,bus-width = <128>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x14eb>;
			power-domains = <&pd_gdma>;
		};

		fpd_dma_chan5: dma@fd540000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			reg = <0x0 0xfd540000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 128 4>;
			clock-names = "clk_main", "clk_apb";
			xlnx,bus-width = <128>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x14ec>;
			power-domains = <&pd_gdma>;
		};

		fpd_dma_chan6: dma@fd550000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			reg = <0x0 0xfd550000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 129 4>;
			clock-names = "clk_main", "clk_apb";
			xlnx,bus-width = <128>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x14ed>;
			power-domains = <&pd_gdma>;
		};

		fpd_dma_chan7: dma@fd560000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			reg = <0x0 0xfd560000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 130 4>;
			clock-names = "clk_main", "clk_apb";
			xlnx,bus-width = <128>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x14ee>;
			power-domains = <&pd_gdma>;
		};

		fpd_dma_chan8: dma@fd570000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			reg = <0x0 0xfd570000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 131 4>;
			clock-names = "clk_main", "clk_apb";
			xlnx,bus-width = <128>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x14ef>;
			power-domains = <&pd_gdma>;
		};

		gpu: gpu@fd4b0000 {
			status = "disabled";
			compatible = "arm,mali-400", "arm,mali-utgard";
			reg = <0x0 0xfd4b0000 0x0 0x30000>;
			interrupt-parent = <&gic>;
			interrupts = <0 132 4>, <0 132 4>, <0 132 4>, <0 132 4>, <0 132 4>, <0 132 4>;
			interrupt-names = "IRQGP", "IRQGPMMU", "IRQPP0", "IRQPPMMU0", "IRQPP1", "IRQPPMMU1";
			power-domains = <&pd_gpu>;
		};

		/* LPDDMA default allows only secured access. inorder to enable
		 * These dma channels, Users should ensure that these dma
		 * Channels are allowed for non secure access.
		 */
		lpd_dma_chan1: dma@ffa80000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			clock-names = "clk_main", "clk_apb";
			reg = <0x0 0xffa80000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 77 4>;
			xlnx,bus-width = <64>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x868>;
			power-domains = <&pd_adma>;
		};

		lpd_dma_chan2: dma@ffa90000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			clock-names = "clk_main", "clk_apb";
			reg = <0x0 0xffa90000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 78 4>;
			xlnx,bus-width = <64>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x869>;
			power-domains = <&pd_adma>;
		};

		lpd_dma_chan3: dma@ffaa0000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			clock-names = "clk_main", "clk_apb";
			reg = <0x0 0xffaa0000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 79 4>;
			xlnx,bus-width = <64>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x86a>;
			power-domains = <&pd_adma>;
		};

		lpd_dma_chan4: dma@ffab0000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			clock-names = "clk_main", "clk_apb";
			reg = <0x0 0xffab0000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 80 4>;
			xlnx,bus-width = <64>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x86b>;
			power-domains = <&pd_adma>;
		};

		lpd_dma_chan5: dma@ffac0000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			clock-names = "clk_main", "clk_apb";
			reg = <0x0 0xffac0000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 81 4>;
			xlnx,bus-width = <64>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x86c>;
			power-domains = <&pd_adma>;
		};

		lpd_dma_chan6: dma@ffad0000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			clock-names = "clk_main", "clk_apb";
			reg = <0x0 0xffad0000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 82 4>;
			xlnx,bus-width = <64>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x86d>;
			power-domains = <&pd_adma>;
		};

		lpd_dma_chan7: dma@ffae0000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			clock-names = "clk_main", "clk_apb";
			reg = <0x0 0xffae0000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 83 4>;
			xlnx,bus-width = <64>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x86e>;
			power-domains = <&pd_adma>;
		};

		lpd_dma_chan8: dma@ffaf0000 {
			status = "disabled";
			compatible = "xlnx,zynqmp-dma-1.0";
			clock-names = "clk_main", "clk_apb";
			reg = <0x0 0xffaf0000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 84 4>;
			xlnx,bus-width = <64>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x86f>;
			power-domains = <&pd_adma>;
		};

		mc: memory-controller@fd070000 {
			compatible = "xlnx,zynqmp-ddrc-2.40a";
			reg = <0x0 0xfd070000 0x0 0x30000>;
			interrupt-parent = <&gic>;
			interrupts = <0 112 4>;
		};

		nand0: nand@ff100000 {
			compatible = "arasan,nfc-v3p10";
			status = "disabled";
			reg = <0x0 0xff100000 0x0 0x1000>;
			clock-names = "clk_sys", "clk_flash";
			interrupt-parent = <&gic>;
			interrupts = <0 14 4>;
			#address-cells = <2>;
			#size-cells = <1>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x872>;
			power-domains = <&pd_nand>;
		};

		gem0: ethernet@ff0b0000 {
			compatible = "cdns,zynqmp-gem";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 57 4>, <0 57 4>;
			reg = <0x0 0xff0b0000 0x0 0x1000>;
			clock-names = "pclk", "hclk", "tx_clk";
			#address-cells = <1>;
			#size-cells = <0>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x874>;
			power-domains = <&pd_eth0>;
		};

		gem1: ethernet@ff0c0000 {
			compatible = "cdns,zynqmp-gem";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 59 4>, <0 59 4>;
			reg = <0x0 0xff0c0000 0x0 0x1000>;
			clock-names = "pclk", "hclk", "tx_clk";
			#address-cells = <1>;
			#size-cells = <0>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x875>;
			power-domains = <&pd_eth1>;
		};

		gem2: ethernet@ff0d0000 {
			compatible = "cdns,zynqmp-gem";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 61 4>, <0 61 4>;
			reg = <0x0 0xff0d0000 0x0 0x1000>;
			clock-names = "pclk", "hclk", "tx_clk";
			#address-cells = <1>;
			#size-cells = <0>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x876>;
			power-domains = <&pd_eth2>;
		};

		gem3: ethernet@ff0e0000 {
			compatible = "cdns,zynqmp-gem";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 63 4>, <0 63 4>;
			reg = <0x0 0xff0e0000 0x0 0x1000>;
			clock-names = "pclk", "hclk", "tx_clk";
			#address-cells = <1>;
			#size-cells = <0>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x877>;
			power-domains = <&pd_eth3>;
		};

		gpio: gpio@ff0a0000 {
			compatible = "xlnx,zynqmp-gpio-1.0";
			status = "disabled";
			#gpio-cells = <0x2>;
			interrupt-parent = <&gic>;
			interrupts = <0 16 4>;
			interrupt-controller;
			#interrupt-cells = <2>;
			reg = <0x0 0xff0a0000 0x0 0x1000>;
			power-domains = <&pd_gpio>;
		};

		i2c0: i2c@ff020000 {
			compatible = "cdns,i2c-r1p10";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 17 4>;
			reg = <0x0 0xff020000 0x0 0x1000>;
			#address-cells = <1>;
			#size-cells = <0>;
			power-domains = <&pd_i2c0>;
		};

		i2c1: i2c@ff030000 {
			compatible = "cdns,i2c-r1p10";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 18 4>;
			reg = <0x0 0xff030000 0x0 0x1000>;
			#address-cells = <1>;
			#size-cells = <0>;
			power-domains = <&pd_i2c1>;
		};

		ocm: memory-controller@ff960000 {
			compatible = "xlnx,zynqmp-ocmc-1.0";
			reg = <0x0 0xff960000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <0 10 4>;
		};

		pcie: pcie@fd0e0000 {
			compatible = "xlnx,nwl-pcie-2.11";
			status = "disabled";
			#address-cells = <3>;
			#size-cells = <2>;
			#interrupt-cells = <1>;
			msi-controller;
			device_type = "pci";
			interrupt-parent = <&gic>;
			interrupts = <0 118 4>,
				     <0 117 4>,
				     <0 116 4>,
				     <0 115 4>,	/* MSI_1 [63...32] */
				     <0 114 4>;	/* MSI_0 [31...0] */
			interrupt-names = "misc","dummy","intx", "msi1", "msi0";
			msi-parent = <&pcie>;
			reg = <0x0 0xfd0e0000 0x0 0x1000>,
			      <0x0 0xfd480000 0x0 0x1000>,
			      <0x80 0x00000000 0x0 0x1000000>;
			reg-names = "breg", "pcireg", "cfg";
			ranges = <0x02000000 0x00000000 0xe0000000 0x00000000 0xe0000000 0x00000000 0x10000000	/* non-prefetchable memory */
				  0x43000000 0x00000006 0x00000000 0x00000006 0x00000000 0x00000002 0x00000000>;/* prefetchable memory */
			interrupt-map-mask = <0x0 0x0 0x0 0x7>;
			interrupt-map = <0x0 0x0 0x0 0x1 &pcie_intc 0x1>,
					<0x0 0x0 0x0 0x2 &pcie_intc 0x2>,
					<0x0 0x0 0x0 0x3 &pcie_intc 0x3>,
					<0x0 0x0 0x0 0x4 &pcie_intc 0x4>;
			power-domains = <&pd_pcie>;
			pcie_intc: legacy-interrupt-controller {
				interrupt-controller;
				#address-cells = <0>;
				#interrupt-cells = <1>;
			};
		};

		qspi: spi@ff0f0000 {
			compatible = "xlnx,zynqmp-qspi-1.0";
			status = "disabled";
			clock-names = "ref_clk", "pclk";
			interrupts = <0 15 4>;
			interrupt-parent = <&gic>;
			num-cs = <1>;
			reg = <0x0 0xff0f0000 0x0 0x1000>,
			      <0x0 0xc0000000 0x0 0x8000000>;
			#address-cells = <1>;
			#size-cells = <0>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x873>;
			power-domains = <&pd_qspi>;
		};

		rtc: rtc@ffa60000 {
			compatible = "xlnx,zynqmp-rtc";
			status = "disabled";
			reg = <0x0 0xffa60000 0x0 0x100>;
			interrupt-parent = <&gic>;
			interrupts = <0 26 4>, <0 27 4>;
			interrupt-names = "alarm", "sec";
		};

		serdes: zynqmp_phy@fd400000 {
			compatible = "xlnx,zynqmp-psgtr";
			status = "disabled";
			reg = <0x0 0xfd400000 0x0 0x40000>,
			      <0x0 0xfd3d0000 0x0 0x1000>,
			      <0x0 0xfd1a0000 0x0 0x1000>,
			      <0x0 0xff5e0000 0x0 0x1000>;
			reg-names = "serdes", "siou", "fpd", "lpd";
			xlnx,tx_termination_fix;
			lane0: lane0 {
				#phy-cells = <4>;
			};
			lane1: lane1 {
				#phy-cells = <4>;
			};
			lane2: lane2 {
				#phy-cells = <4>;
			};
			lane3: lane3 {
				#phy-cells = <4>;
			};
		};

		sata: ahci@fd0c0000 {
			compatible = "ceva,ahci-1v84";
			status = "disabled";
			reg = <0x0 0xfd0c0000 0x0 0x2000>;
			interrupt-parent = <&gic>;
			interrupts = <0 133 4>;
			power-domains = <&pd_sata>;
		};

		sdhci0: sdhci@ff160000 {
			u-boot,dm-pre-reloc;
			compatible = "xlnx,zynqmp-8.9a", "arasan,sdhci-8.9a";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 48 4>;
			reg = <0x0 0xff160000 0x0 0x1000>;
			clock-names = "clk_xin", "clk_ahb";
			xlnx,device_id = <0>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x870>;
			power-domains = <&pd_sd0>;
		};

		sdhci1: sdhci@ff170000 {
			u-boot,dm-pre-reloc;
			compatible = "xlnx,zynqmp-8.9a", "arasan,sdhci-8.9a";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 49 4>;
			reg = <0x0 0xff170000 0x0 0x1000>;
			clock-names = "clk_xin", "clk_ahb";
			xlnx,device_id = <1>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x871>;
			power-domains = <&pd_sd1>;
		};

		smmu: smmu@fd800000 {
			compatible = "arm,mmu-500";
			reg = <0x0 0xfd800000 0x0 0x20000>;
			#iommu-cells = <1>;
			#global-interrupts = <1>;
			interrupt-parent = <&gic>;
			interrupts = <0 155 4>,
				<0 155 4>, <0 155 4>, <0 155 4>, <0 155 4>,
				<0 155 4>, <0 155 4>, <0 155 4>, <0 155 4>,
				<0 155 4>, <0 155 4>, <0 155 4>, <0 155 4>,
				<0 155 4>, <0 155 4>, <0 155 4>, <0 155 4>;
			mmu-masters = < &gem0 0x874
					&gem1 0x875
					&gem2 0x876
					&gem3 0x877
					&usb0 0x860
					&usb1 0x861
					&qspi 0x873
					&lpd_dma_chan1 0x868
					&lpd_dma_chan2 0x869
					&lpd_dma_chan3 0x86a
					&lpd_dma_chan4 0x86b
					&lpd_dma_chan5 0x86c
					&lpd_dma_chan6 0x86d
					&lpd_dma_chan7 0x86e
					&lpd_dma_chan8 0x86f
					&fpd_dma_chan1 0x14e8
					&fpd_dma_chan2 0x14e9
					&fpd_dma_chan3 0x14ea
					&fpd_dma_chan4 0x14eb
					&fpd_dma_chan5 0x14ec
					&fpd_dma_chan6 0x14ed
					&fpd_dma_chan7 0x14ee
					&fpd_dma_chan8 0x14ef
					&sdhci0 0x870
					&sdhci1 0x871
					&nand0 0x872>;
		};

		spi0: spi@ff040000 {
			compatible = "cdns,spi-r1p6";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 19 4>;
			reg = <0x0 0xff040000 0x0 0x1000>;
			clock-names = "ref_clk", "pclk";
			#address-cells = <1>;
			#size-cells = <0>;
			power-domains = <&pd_spi0>;
		};

		spi1: spi@ff050000 {
			compatible = "cdns,spi-r1p6";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 20 4>;
			reg = <0x0 0xff050000 0x0 0x1000>;
			clock-names = "ref_clk", "pclk";
			#address-cells = <1>;
			#size-cells = <0>;
			power-domains = <&pd_spi1>;
		};

		ttc0: timer@ff110000 {
			compatible = "cdns,ttc";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 36 4>, <0 37 4>, <0 38 4>;
			reg = <0x0 0xff110000 0x0 0x1000>;
			timer-width = <32>;
			power-domains = <&pd_ttc0>;
		};

		ttc1: timer@ff120000 {
			compatible = "cdns,ttc";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 39 4>, <0 40 4>, <0 41 4>;
			reg = <0x0 0xff120000 0x0 0x1000>;
			timer-width = <32>;
			power-domains = <&pd_ttc1>;
		};

		ttc2: timer@ff130000 {
			compatible = "cdns,ttc";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 42 4>, <0 43 4>, <0 44 4>;
			reg = <0x0 0xff130000 0x0 0x1000>;
			timer-width = <32>;
			power-domains = <&pd_ttc2>;
		};

		ttc3: timer@ff140000 {
			compatible = "cdns,ttc";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 45 4>, <0 46 4>, <0 47 4>;
			reg = <0x0 0xff140000 0x0 0x1000>;
			timer-width = <32>;
			power-domains = <&pd_ttc3>;
		};

		uart0: serial@ff000000 {
			u-boot,dm-pre-reloc;
			compatible = "cdns,uart-r1p12", "xlnx,xuartps";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 21 4>;
			reg = <0x0 0xff000000 0x0 0x1000>;
			clock-names = "uart_clk", "pclk";
			power-domains = <&pd_uart0>;
		};

		uart1: serial@ff010000 {
			u-boot,dm-pre-reloc;
			compatible = "cdns,uart-r1p12", "xlnx,xuartps";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 22 4>;
			reg = <0x0 0xff010000 0x0 0x1000>;
			clock-names = "uart_clk", "pclk";
			power-domains = <&pd_uart1>;
		};

		usb0: usb0 {
			#address-cells = <2>;
			#size-cells = <2>;
			status = "disabled";
			compatible = "xlnx,zynqmp-dwc3";
			clock-names = "bus_clk", "ref_clk";
			clocks = <&clk125>, <&clk125>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x860>;
			power-domains = <&pd_usb0>;
			ranges;

			dwc3_0: dwc3@fe200000 {
				compatible = "snps,dwc3";
				status = "disabled";
				reg = <0x0 0xfe200000 0x0 0x40000>;
				interrupt-parent = <&gic>;
				interrupts = <0 65 4>;
				/* snps,quirk-frame-length-adjustment = <0x20>; */
				snps,refclk_fladj;
			};
		};

		usb1: usb1 {
			#address-cells = <2>;
			#size-cells = <2>;
			status = "disabled";
			compatible = "xlnx,zynqmp-dwc3";
			clock-names = "bus_clk", "ref_clk";
			clocks = <&clk125>, <&clk125>;
			#stream-id-cells = <1>;
			iommus = <&smmu 0x861>;
			power-domains = <&pd_usb1>;
			ranges;

			dwc3_1: dwc3@fe300000 {
				compatible = "snps,dwc3";
				status = "disabled";
				reg = <0x0 0xfe300000 0x0 0x40000>;
				interrupt-parent = <&gic>;
				interrupts = <0 70 4>;
				/* snps,quirk-frame-length-adjustment = <0x20>; */
				snps,refclk_fladj;
			};
		};

		watchdog0: watchdog@fd4d0000 {
			compatible = "cdns,wdt-r1p2";
			status = "disabled";
			interrupt-parent = <&gic>;
			interrupts = <0 113 1>;
			reg = <0x0 0xfd4d0000 0x0 0x1000>;
			timeout-sec = <10>;
		};

		xilinx_drm: xilinx_drm {
			compatible = "xlnx,drm";
			status = "disabled";
			xlnx,encoder-slave = <&xlnx_dp>;
			xlnx,connector-type = "DisplayPort";
			xlnx,dp-sub = <&xlnx_dp_sub>;
			planes {
				xlnx,pixel-format = "rgb565";
				plane0 {
					dmas = <&xlnx_dpdma 3>;
					dma-names = "dma0";
				};
				plane1 {
					dmas = <&xlnx_dpdma 0>,
					       <&xlnx_dpdma 1>,
					       <&xlnx_dpdma 2>;
					dma-names = "dma0", "dma1", "dma2";
				};
			};
		};

		xlnx_dp: dp@fd4a0000 {
			compatible = "xlnx,v-dp";
			status = "disabled";
			reg = <0x0 0xfd4a0000 0x0 0x1000>;
			interrupts = <0 119 4>;
			interrupt-parent = <&gic>;
			clock-names = "aclk", "aud_clk";
			xlnx,dp-version = "v1.2";
			xlnx,max-lanes = <2>;
			xlnx,max-link-rate = <540000>;
			xlnx,max-bpc = <16>;
			xlnx,enable-ycrcb;
			xlnx,colormetry = "rgb";
			xlnx,bpc = <8>;
			xlnx,audio-chan = <2>;
			xlnx,dp-sub = <&xlnx_dp_sub>;
			xlnx,max-pclock-frequency = <300000>;
		};

		xlnx_dp_snd_card: dp_snd_card {
			compatible = "xlnx,dp-snd-card";
			status = "disabled";
			xlnx,dp-snd-pcm = <&xlnx_dp_snd_pcm0>, <&xlnx_dp_snd_pcm1>;
			xlnx,dp-snd-codec = <&xlnx_dp_snd_codec0>;
		};

		xlnx_dp_snd_codec0: dp_snd_codec0 {
			compatible = "xlnx,dp-snd-codec";
			status = "disabled";
			clock-names = "aud_clk";
		};

		xlnx_dp_snd_pcm0: dp_snd_pcm0 {
			compatible = "xlnx,dp-snd-pcm";
			status = "disabled";
			dmas = <&xlnx_dpdma 4>;
			dma-names = "tx";
		};

		xlnx_dp_snd_pcm1: dp_snd_pcm1 {
			compatible = "xlnx,dp-snd-pcm";
			status = "disabled";
			dmas = <&xlnx_dpdma 5>;
			dma-names = "tx";
		};

		xlnx_dp_sub: dp_sub@fd4aa000 {
			compatible = "xlnx,dp-sub";
			status = "disabled";
			reg = <0x0 0xfd4aa000 0x0 0x1000>,
			      <0x0 0xfd4ab000 0x0 0x1000>,
			      <0x0 0xfd4ac000 0x0 0x1000>;
			reg-names = "blend", "av_buf", "aud";
			xlnx,output-fmt = "rgb";
			xlnx,vid-fmt = "yuyv";
			xlnx,gfx-fmt = "rgb565";
		};

		xlnx_dpdma: dma@fd4c0000 {
			compatible = "xlnx,dpdma";
			status = "disabled";
			reg = <0x0 0xfd4c0000 0x0 0x1000>;
			interrupts = <0 122 4>;
			interrupt-parent = <&gic>;
			clock-names = "axi_clk";
			dma-channels = <6>;
			#dma-cells = <1>;
			dma-video0channel {
				compatible = "xlnx,video0";
			};
			dma-video1channel {
				compatible = "xlnx,video1";
			};
			dma-video2channel {
				compatible = "xlnx,video2";
			};
			dma-graphicschannel {
				compatible = "xlnx,graphics";
			};
			dma-audio0channel {
				compatible = "xlnx,audio0";
			};
			dma-audio1channel {
				compatible = "xlnx,audio1";
			};
		};
	};
};
