/*
 * Device Tree Include file for Marvell Armada 388 SoC.
 *
 * Copyright (C) 2015 Marvell
 *
 * Gregory CLEMENT <gregory.clement@free-electrons.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is licensed under the terms of the GNU General Public
 *     License version 2.  This program is licensed "as is" without
 *     any warranty of any kind, whether express or implied.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 *
 *
 * The main difference with the Armada 385 is that the 388 can handle two more
 * SATA ports. So we can reuse the dtsi of the Armada 385, override the pinctrl
 * property and the name of the SoC, and add the second SATA host which control
 * the 2 other ports.
 */

#include "armada-385.dtsi"

/ {
	model = "Marvell Armada 388 family SoC";
	compatible = "marvell,armada388", "marvell,armada385",
		"marvell,armada380";

	soc {
		internal-regs {
			pinctrl@18000 {
				compatible = "marvell,mv88f6828-pinctrl";
			};

			sata@e0000 {
				compatible = "marvell,armada-380-ahci";
				reg = <0xe0000 0x2000>;
				interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gateclk 30>;
				status = "disabled";
			};

		};
	};
};
