/*
 * Copyright (C) 2014 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 * Based on "omap4.dtsi"
 */

#include "dra7.dtsi"

/ {
	compatible = "ti,dra722", "ti,dra72", "ti,dra7";

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <0>;

			/* cooling options */
			cooling-min-level = <0>;
			cooling-max-level = <2>;
			#cooling-cells = <2>; /* min followed by max */
		};
	};

	pmu {
		compatible = "arm,cortex-a15-pmu";
		interrupt-parent = <&wakeupgen>;
		interrupts = <GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>;
	};
};

&dss {
	reg = <0x58000000 0x80>,
	      <0x58004054 0x4>,
	      <0x58004300 0x20>;
	reg-names = "dss", "pll1_clkctrl", "pll1";

	clocks = <&dss_dss_clk>,
		 <&dss_video1_clk>;
	clock-names = "fck", "video1_clk";
};
