/*
 * Copyright 2014 Chen-Yu Tsai
 *
 * Chen-Yu Tsai <wens@csie.org>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

#include "sun8i-a23-a33.dtsi"

/ {
	memory {
		reg = <0x40000000 0x40000000>;
	};

	clocks {
		ahb1_gates: clk@01c20060 {
			#clock-cells = <1>;
			compatible = "allwinner,sun8i-a23-ahb1-gates-clk";
			reg = <0x01c20060 0x8>;
			clocks = <&ahb1>;
			clock-indices = <1>, <6>,
					<8>, <9>, <10>,
					<13>, <14>,
					<19>, <20>,
					<21>, <24>, <26>,
					<29>, <32>, <36>,
					<40>, <44>, <46>,
					<52>, <53>,
					<54>, <57>;
			clock-output-names = "ahb1_mipidsi", "ahb1_dma",
					"ahb1_mmc0", "ahb1_mmc1", "ahb1_mmc2",
					"ahb1_nand", "ahb1_sdram",
					"ahb1_hstimer", "ahb1_spi0",
					"ahb1_spi1", "ahb1_otg", "ahb1_ehci",
					"ahb1_ohci", "ahb1_ve", "ahb1_lcd",
					"ahb1_csi", "ahb1_be",	"ahb1_fe",
					"ahb1_gpu", "ahb1_msgbox",
					"ahb1_spinlock", "ahb1_drc";
		};

		mbus_clk: clk@01c2015c {
			#clock-cells = <0>;
			compatible = "allwinner,sun8i-a23-mbus-clk";
			reg = <0x01c2015c 0x4>;
			clocks = <&osc24M>, <&pll6 1>, <&pll5>;
			clock-output-names = "mbus";
		};
	};

	soc@01c00000 {
		usb_otg: usb@01c19000 {
			compatible = "allwinner,sun6i-a31-musb";
			reg = <0x01c19000 0x0400>;
			clocks = <&ahb1_gates 24>;
			resets = <&ahb1_rst 24>;
			interrupts = <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "mc";
			phys = <&usbphy 0>;
			phy-names = "usb";
			extcon = <&usbphy 0>;
			status = "disabled";
		};

		usbphy: phy@01c19400 {
			compatible = "allwinner,sun8i-a23-usb-phy";
			reg = <0x01c19400 0x10>,
			      <0x01c1a800 0x4>;
			reg-names = "phy_ctrl",
				    "pmu1";
			clocks = <&usb_clk 8>,
				 <&usb_clk 9>;
			clock-names = "usb0_phy",
				      "usb1_phy";
			resets = <&usb_clk 0>,
				 <&usb_clk 1>;
			reset-names = "usb0_reset",
				      "usb1_reset";
			status = "disabled";
			#phy-cells = <1>;
		};
	};
};

&pio {
	compatible = "allwinner,sun8i-a23-pinctrl";
	interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>,
		     <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>;
};
